## HIOKI IM7580A, IM7581, IM7583, IM7585 and IM7587 Impedance Analyzer Instrument Driver Readme

To rate this instrument driver, go to the driver download page on the Instrument Driver Network.

#### 1. Overview

Instrument Driver Technology: LabVIEW Plug and Play (project-style)
Manufacturer: HIOKI
Supported Language(s): LabVIEW
Supported Model(s): IM7580A, IM7581, IM7583, IM7585, IM7587
Model(s) Tested: IM7580A, IM7581, IM7583, IM7585, IM7587
Interface(s): GPIB, RS232C, USB, LAN
Firmware Revision(s) Tested: 1.00
Driver Revision: 1.2
Original Release Date: 08/01/2015
Current Revision Date: 09/01/2016

#### 2. Required Software

Some software components need to be installed before using this instrument driver. The minimum versions of these components are listed below, and can be downloaded from the Download Site.
VISA 14.0 or later
LabVIEW 2015 or later
Refer to the LabVIEW Help for more information about software requirements. You access the LabVIEW Help by selecting Help»Search the LabVIEW Help.

#### 3. Installation Instructions

LabVIEW: Instrument drivers should be installed as a subdirectory of the LabVIEW\instr.lib. The HIOKI IM7580A, IM7581, IM7583, IM7585 and IM7587 Impedance Analyzer instrument driver is installed in the following directory:
LabVIEW\instr.lib\HIOKI IM758x

#### 4. Known Issues

To report issues or provide feedback about this instrument driver, please send an email to instrument.drivers@ni.com.

#### 5. Revision History

The latest version of this and other LabVIEW and LabWindows/CVI instrument drivers can be downloaded at the Instrument Driver Network.
REV 1.0, LV 2014, 08/01/2015
Original Release.
REV 1.1, LV 2015, 12/01/2015
Correspond to IM7580A and IM7581.
REV 1.2, LV 2015, 09/01/2016
Correspond to IM7587.