Sample Program 3

This program establishes a connection with the instrument and reads the measurement value of each CH and pastes it into Microsoft Office Excel (hereinafter referred to as Excel).
The setting item is the setting for writing to Excel. This is not a setting for this instrument.
The interval between data retrieval can be set to one second or more.
To use this program, you must have Excel installed.
LAN Example program
USB Example program