Comments (COMMent)

Sets and queries the comment characters for alarm channel.
Syntax | (Command) (Query) | :COMMent:ALMCH alm$,"A$" :COMMent:ALMCH? alm$
(Response) | alm$,"A$" alm$ = A$ = comment characters (up to 40 characters)
Details | Sets a string of comment characters for the alarm channel specified by alm$. Returns a string of comment characters for the alarm channel specified by alm$ as character data. Single quotation marks (') can be used instead of double quotation marks("). Entry of the special characters is as follows.
PC | ^2 | ^3 | ~u | ~o | ~e | ~c | ~+ | ~, | ~; | ^^ | ~~
LR8450 LR8450-01 | 2 | 3 | μ | Ω | ε | ° | ± | ' | " | ^ | ~
Example | :COMMent:ALMCH ALM1,"ABCDEFG" :COMMent:ALMCH? ALM1 (Response) :COMMENT:ALMCH ALM1,"ABCDEFG" (when headers are enabled)
Note | Characters exceeding the maximum number of characters are not set. The alarm channel comment settings cannot be changed during measurement.
Usage Conditions | -

Sets and queries the comment characters for each channel.
Syntax | (Command) (Query) | :COMMent:CH ch$,"A$" :COMMent:CH? ch$
(Response) | ch$,"A$" ch$ = , , A$ = comment characters (up to 40 characters)
Details | Sets a string of comment characters for the channel specified by ch$. Returns a string of comment characters for the channel specified by ch$ as character data. Single quotation marks (') can be used instead of double quotation marks("). Entry of the special characters is as follows.
PC | ^2 | ^3 | ~u | ~o | ~e | ~c | ~+ | ~, | ~; | ^^ | ~~
LR8450 LR8450-01 | 2 | 3 | μ | Ω | ε | ° | ± | ' | " | ^ | ~
Example | :COMMent:CH CH1_1,"ABCDEFG" :COMMent:CH? CH1_1 (Response) :COMMENT:CH CH1_1,"ABCDEFG" (when headers are enabled)
Note | Characters exceeding the maximum number of characters are not set. The channel comment settings cannot be changed during measurement.
Usage Conditions | -

Sets and queries the title comments, and inputs comment characters.
Syntax | (Command) (Query) | :COMMent:TITLe "A$" :COMMent:TITLe?
(Response) | "A$" A$ = comment characters (up to 40 characters)
Details | Sets a string of title comment characters. Returns a string of title comment characters as character data. Single quotation marks (') can be used instead of double quotation marks("). Entry of the special characters is as follows.
PC | ^2 | ^3 | ~u | ~o | ~e | ~c | ~+ | ~, | ~; | ^^ | ~~
LR8450 LR8450-01 | 2 | 3 | μ | Ω | ε | ° | ± | ' | " | ^ | ~
Example | :COMMent:TITLe "HIOKI" :COMMent:TITLe? (Response) :COMMENT:TITLE "HIOKI" (when headers are enabled)
Note | Characters exceeding the maximum number of characters are not set. The title comment settings cannot be changed during measurement.
Usage Conditions | -

Sets and queries the identifier characters for each unit.
Syntax | (Command) (Query) | :COMMent:UNIT unit$,"A$" :COMMent:UNIT? unit$
(Response) | unit$,"A$" unit$ = A$ = identifier characters (up to 16 characters)
Details | Sets a string of identifier characters for the each unit specified by unit$. Returns a string of identifier characters for the each unit specified by unit$ as character data. Single quotation marks (') can be used instead of double quotation marks("). Entry of the special characters is as follows.
PC | ^2 | ^3 | ~u | ~o | ~e | ~c | ~+ | ~, | ~; | ^^ | ~~
LR8450 LR8450-01 | 2 | 3 | μ | Ω | ε | ° | ± | ' | " | ^ | ~
Example | :COMMent:UNIT UNIT1,"ABCDEFG" :COMMent:UNIT? UNIT1 (Response) :COMMENT:UNIT UNIT1,"ABCDEFG" (when headers are enabled)
Note | Characters exceeding the maximum number of characters are not set. The identifier characters for each unit cannot be changed during measurement.
Usage Conditions | -