Environment (SYSTem)

Command | Data (for a query, response data) | Explanation
:ADDComment A$ | A$ = OFF, ON | Sets title comment addition for manual save file name Queries
:ADDComment? | A$
:ADDDate A$ | A$ = OFF, ON | Sets trigger date addition for manual save file name Queries
:ADDDate? | A$
:AUTOStart A$ | A$ = OFF, ON | Sets auto start measurement Queries
:AUTOStart? | A$
:BATT? unit$ | unit$,A$ unit$ = REMOTE1 to REMOTE7, MAIN1, MAIN2 [unit$ = REMOTE1 to REMOTE7] A$ = EMPTY, LEVEL_L, LEVEL_M, LEVEL_H, AC [unit$ = MAIN1, MAIN2] A$ = EMPTY, LEVEL_L, LEVEL_M, LEVEL_H, NOBATTERY, AC, CHARGE | Queries power supply state
:BEEP A$ | A$ = OFF, ON | Sets beep sound Queries
:BEEP? | A$
:BRIGhtness A$ | A$ = LV1, LV2, LV3, LV4, LV5 | Sets the backlight brightness Queries
:BRIGhtness? | A$
:CALCSplit A$ | A$ = OFF, ON | Sets calculation file divisionses for manual saving. Queries
:CALCSplit? | A$
:CHECk | - | Executes ROM/RAM check Queries the result
:CHECk? | A$ = NONE, RUN, PASS, FAIL
:CRTOff A$ | A$ = OFF, 30S, 1MIN, 2MIN, 5MIN, 10MIN | Sets the backlight saver Queries
:CRTOff? | A$
:DATAClear | - | Clear waveform data
:DATE year,month,day | year = 0 to 37 month = 1 to 12 day = 1 to 31 | Sets the calendar Queries
:DATE? | year<NR1>,month<NR1>,day<NR1>
:DATETime year,month,day,hour,minute,second | year = 0 to 37 month = 1 to 12 day = 1 to 31 hour = 0 to 23 minute = 0 to 59 second = 0 to 59 | Sets the date and time Queries
:DATETime? | year<NR1>,month<NR1>,day<NR1> hour<NR1>,minute<NR1>,second<NR1>
:DFORmat A$ | A$ = YYYYMMDD ,MMDDYYYY ,DDMMYYYY | Sets the date format Queries
:DFORmat? | A$
:DSEParator A$ | A$ = HYPHEN ,SLASH ,PERIOD | Sets the date separator character. Queries
:DSEParator? | A$
:FILEName "A$" | A$ = file name(8 character) | Sets file name for manual save Queries
:FILEName? | "A$"
:KEYMap A$ | A$ = JP ,US ,CN ,FR ,ES ,DE ,IT | Sets Key Map Queries
:KEYMap? | A$
:LANGuage A$ | A$ = JAPANese, ENGlish, CHINese, KORean, TRADitionalchinese | Sets the language Queries
:LANGuage? | A$
:MARK A$ | A$ = OFF, ON | Sets event mark at alarm Queries
:MARK? | A$
:RETRansmit? A$ | r1,r2,r3,r4,r5,r6,r7 A$ = RECent,WORSt r1～r7 = -1(NO DATA),0.0~100.0 | Queries the wireless unit retransmit-rate
:RSSI? unit$ | unit$,A<NR1> unit$ = REMOTE1 to REMOTE7 A = Radio field strength by the side of a main unit(db) | Queries radio field strength
:SAVEFormat A$ | A$ = BINARY, CSV, MF4 | Sets wave file format Queries
:SAVEFormat? | A$
:SAVEKey A$ | A$ = SELECT, QUICK | Sets save key operation Queries
:SAVEKey? | A$
:SAVEPri A$ | A$ = SD, USB | Sets manual save priority Queries
:SAVEpri? | A$
:SAVESpan A$ | A$ = ALL, A-B, START-A, START-B, A-END, B-END | Sets wave file span Queries
:SAVESpan? | A$
:SAVEType A$ | A$ = WAVE, IMAGE, SET, CALC, A2L | Sets save type Queries
:SAVEType? | A$
:SMESS A$ | A$ = OFF, ON | Sets operation error prevention function Queries
:SMESS? | A$
:STARt A$ | A$ = OFF, ON | Sets start backup
:STARt? | A$
:THINData A$ | A$ = INSTANT, STATISTICS | Sets downsampling type for manual save Queries
:THINData? | A$
:THINOut A | A = 1(OFF) to 100000 | Sets decimation factor for manual save Queries
:THINOut? | A<NR1>
:TIME h,m,s | h = 0 to 23 m = 0 to 59 s = 0 to 59 | Sets the time Queries
:TIME? | hh<NR1>,mm<NR1>,ss<NR1>
:TIMEZone hour(,min) | hour = -12 to +14 min = 30, 45 | Sets the time zone Queries
:TIMEZone? | hour<NR1>(,min<NR1>)
:TMAXis A$ | A$ = TIME, DATE, SCALe | Sets the time axis display Queries
:TMAXis? | A$
:UNITCheck? A$ | [A$ = DIRect] u1u2u3u4 [A$ = REMote] r1r2r3r4r5r6r7 u1~u4,r1~r7 = 0(OK),1(NG),*(no unit) A$ = DIRect,REMote | Execute the unit SRAM check and query the result
:VOUT out$,A$ | out$ = OUT1, OUT2 A$ = OFF, 5V, 12V, 24V | Sets voltage output Queries
:VOUT? out$ | out$,A$
:WAVEBackcolor A$ | A$ = DARK, LIGHT | Sets waveform background color Queries
:WAVEBackcolor | A$
External Tarminals (:SYSTem:EXT)
External input 1[I/O 1](:SYSTem:EXT:IO1)
:KIND A$ | A$ = OFF, STARTIN, STOPIN, S_SIN, EVENTIN | Sets input kind Queries
:KIND? | A$
:SLOPe:STARt A$ | A$ = UP,DOWN | Sets start slope Queries
:SLOPe:STARt? | A$
:SLOPe:STOP A$ | A$ = UP,DOWN | Sets stop slope Queries
:SLOPe:STOP? | A$
External input 2[I/O 2](:SYSTem:EXT:IO2)
:KIND A$ | A$ = OFF, STARTIN, STOPIN, S_SIN, EVENTIN | Sets input kind Queries
:KIND? | A$
:SLOPe:STARt A$ | A$ = UP,DOWN | Sets start slope Queries
:SLOPe:STARt? | A$
:SLOPe:STOP A$ | A$ = UP,DOWN | Sets stop slope Queries
:SLOPe:STOP? | A$
External input 3[I/O 3](:SYSTem:EXT:IO3)
:KIND A$ | A$ = OFF, TRIGIN, EVENTIN | Sets input kind Queries
:KIND? | A$
:SLOPe:STARt A$ | A$ = UP,DOWN | Sets start slope Queries
:SLOPe:STARt? | A$
:SLOPe:STOP A$ | A$ = UP,DOWN | Sets stop slope Queries
:SLOPe:STOP? | A$
External output[I/O 4](:SYSTem:EXT:IO4)
:KIND A$ | A$ = OFF, TRIGOUT | Sets output kind Queries
:KIND? | A$
NTP client function (:SYSTem:NTP)
:ADDRess "A$" | A$ = NTP Server Address(64 characters) | Sets NTP server address Queries
:ADDRess? | A$
:CHECk? | A = 0,1 | Execute the NTP time synchronization and query the result
:KIND A$ | A$ = OFF, ON | Sets NTP client function Queries
:KIND? | A$
:SYNC A$ | A$ = OFF,HOUR,DAY | Sets timing of NTP synchronization Queries
:SYNC? | A$
:STARt A$ | A$ = OFF,ON | Sets the NTP synchronization before start measuring Queries
:STARt? | A$
FTP data auto send setting(:SYSTem:FTP)
:ADDRess "A$" | A$ = FTP server address(45 characters) | Sets the FTP server address for FTP data auto send Queries
:ADDRess? | "A$"
:AUTODel A$ | A$ = OFF, ON | Sets the Deletion of Sent File Queries
:AUTODel? | A$
:CERTificate A$ | A$ = OFF, ON | Sets the verify certificate Queries
:CERTificate? | A$
:CHECk? | A = 0,1 | Execute the unit FTP data send test and query the result
:DIR "A$" | A$ = Destination Directory(45 characters) | Sets the Directory for FTP data auto send Queries
:DIR? | "A$"
:FILE:HOST A$ | A$ = OFF, ON | Sets the Filename identifier(HOST name) Queries
:FILE:HOST? | A$
:FILE:IP A$ | A$ = OFF, ON | Sets the Filename identifier(IP address) Queries
:FILE:IP? | A$
:FILE:TIME A$ | A$ = OFF, ON | Sets the Filename identifier(TIME) Queries
:FILE:TIME? | A$
:PASSword "A$" | A$ = Password(32 characters) | Sets the Password for FTP data auto send Queries
:PASSword? "A$" | B = PASS,FAIL
:PASV A$ | A$ = OFF, ON | Sets the Passive mode for FTP data auto send Queries
:PASV? | A$
:PORT A | A = Port Number(0~65535) | Sets the Port number for FTP data auto send Queries
:PORT? | A<NR1>
:PROG? | A$ = YES,NO | Queries whether there are unsent files
:SECUrity A$ | A$ = OFF, EXPLICIT, IMPLICIT | Sets the connection security Queries
:SECUrity? | A$
:STATe? | A<NR1>, B<NR1>, C<NR1>, D<NR1> A = Number of total files B = Number of sent files C = Number of failes files to send D = Number of unsent files | Queries FTP communication status
:USE A$ | A$ = OFF, ON | Sets the FTP data auto send Queries
:USE? | A$
:USER "A$" | A$ = User Name(32 characters) | Sets the User Name for FTP data auto send Queries
:USER? | "A$"
Execute file loads (:SYSTem:LOAD)
Execute setting conditions file loads (:SYSTem:LOAD:SET)
:SD? "A$",B | C<NR1> A$ = Setting conditions file name(xxx.SET) B = 0 to 3(Load option) C = 0(PASS),1(FAIL) | Execute the Setting conditions file load in the SD card and queries the result
:USB? "A$",B | C<NR1> A$ = Setting conditions file name(xxx.SET) B = 0 to 3(Load option) C = 0(PASS),1(FAIL) | Execute the Setting conditions file load in the USB flash drive and queries the result