Screen (DISPlay)

Command | Data (for a query, response data) | Explanation
:CHANge A$(,B$,C$) | A$ = WAVE,SET,FILE,MONITOR B$ = UNIT,MEAS,CHANNEL,TRIG,ALARM,CALC SYSTEM,SD,USB C$ = RECORD,A_SAVE,M_SAVE,DISPLAY SETTING,CAN,INDIVIDUAL UNIT1,UNIT2,UNIT3,UNIT4 REMOTE1,REMOTE2,REMOTE3,REMOTE4 REMOTE5,REMOTE6,REMOTE7 PULSE,COMMON,W_CALC,ALARM1_8 NUMERICAL,WAVEFORM,XY ENVIRONMENT,INTERFACE,EXTERNAL | Sets the screen mode Queries
:CHANge? | A$
:GAUGe A$ | A$ = OFF, ONE, TWO | Set the number of gauges
:GAUGe? | A$ | Queries the number of gauges
:GCHAn A$,ch$ | A$ = GAUGEA, GAUGEB ch$ = , , | Sets the channel settings for the gauge.
:GCHAn? A$ | A$,ch$ | Queries the Gauge channel
:MARK | - | Insert event mark
:MARK? | A<NR1> A = 0 to 1000 | Queries the event mark num
:MARKJump A | A = 1 to event mark num | Jump to event mark
:MARKJump? A | A<NR1>,B<NR1> A = 1 to event mark num B = data num | Queries the data num at the event mark designeated
:UPDAte A$ | A$ = TRUE, FALSe, REFResh | Sets whether to refresh the screen
:WAVE A$ | A$ = ACUR,TRIG,POINT | Executes waveform
Analog Channel(:DISPlay:ANALog)
:DIGIt ch$,A | ch$ = A = 0 to 10 | Sets the number of digits after the decimal point Queries
:DIGIt? ch$ | ch$,A
:DRAWing ch$,A$ | ch$ = A$ = OFF, C1 to C24 | Sets waveform display color Queries
:DRAWing? ch$ | ch$,A$
:USECh ch$,A$ | ch$ = A$ = OFF, ON | Sets analog waveform display ON/OFF Queries
:USECh? ch$ | ch$,A$
:VARIable ch$,A$ | ch$ = A$ = OFF, ON | Sets upper-lower mode Queries
:VARIable? ch$ | ch$,A$
:VARIUPLOw ch$,A,B | ch$ = A = -9.9999E+29 to 9.9999E+29 (upper level) B = -9.9999E+29 to 9.9999E+29 (lower level) | Sets upper-lower level Queries
:VARIUPLOw? ch$ | ch$,A<NR3>,B<NR3>
:YMAG ch$,A$ | ch$ = A$ = X1_2, X1, X2, X5, X10, X20, X50, X100 | Sets the magnification/compression ratio on the voltage axis Queries
:YMAG? ch$ | ch$,A$
Pulse Channel (:DISPlay:PULSe)
:DIGIt pls$,A | pls$ = A = 0 to 10 | Sets the number of digits after the decimal point Queries
:DIGIt? pls$ | pls$,A
:DRAWing pls$,A$ | pls$ = A$ = OFF, C1 to C24 | Sets waveform display color Queries
:DRAWing? pls$ | pls$,A$
:USECh pls$,A$ | pls$ = A$ = OFF, ON | Sets analog waveform display ON/OFF Queries
:USECh? pls$ | pls$,A$
:VARIable pls$,A$ | pls$ = A$ = OFF, ON | Sets upper-lower mode Queries
:VARIable? pls$ | pls$,A$
:VARIUPLOw pls$,A,B | pls$ = A = -9.9999E+29 to 9.9999E+29 (upper level) B = -9.9999E+29 to 9.9999E+29 (lower level) | Sets upper-lower level Queries
:VARIUPLOw? pls$ | pls$,A<NR3>,B<NR3>
:YMAG pls$,A$ | pls$ = A$ = X1_2, X1, X2, X5, X10, X20, X50, X100 | Sets the magnification/compression ratio on the voltage axis Queries
:YMAG? pls$ | pls$,A$
Alarm Channel (:DISPlay:ALARm)
:DRAWing alm$,A$ | alm$ = A$ = OFF, C1 to C24 | Sets waveform display color Queries
:DRAWing? alm$ | alm$,A$
:USECh alm$,A$ | alm$ = A$ = OFF, ON | Sets analog waveform display ON/OFF Queries
:USECh? alm$ | alm$,A$
Waveform Calculation (:DISPlay:CALCulate)
:DIGIt w$,A | w$ = A = 0 to 10 | Sets the number of digits after the decimal point Queries
:DIGIt? w$ | w$,A
:DRAWing w$,A$ | w$ = A$ = OFF, C1 to C24 | Sets waveform display color Queries
:DRAWing? w$ | w$,A$
:USECh w$,A$ | w$ = A$ = OFF, ON | Sets analog waveform display ON/OFF Queries
:USECh? w$ | w$,A$
:VARIUPLOw w$,A,B | w$ = A = -9.9999E+29 to 9.9999E+29 (upper level) B = -9.9999E+29 to 9.9999E+29 (lower level) | Sets upper-lower level Queries
:VARIUPLOw? w$ | w$,A<NR3>,B<NR3>
XY Synthesis (:DISPlay:XY)
:DRAWing xy$,A$ | xy$ = A$ = OFF, C1 to C24 | Sets waveform display color Queries
:DRAWing? xy$ | xy$,A$
:GAUGe A$ | A$ = OFF, ON | Sets the display of XY gauges Queries
:GAUGe? | A$
:GCHAn xy$ | xy$ = | Sets the channel settings for the XY gauge. Queries
:GCHAn? | xy$
:USECh xy$,A$ | xy$ = A$ = OFF, ON | Sets analog waveform display ON/OFF Queries
:USECh? xy$ | xy$,A$
:XAXIs xy$,ch$ | xy$ = ch$ = ,, | Sets the X-axis channel. Queries
:XAXIs? xy$ | xy$,ch$
:YAXIs xy$,ch$ | xy$ = ch$ = ,, | Sets the Y-axis channel. Queries
:YAXIs? xy$ | xy$,ch$