## About Data Transmission Formats

There is also long format mode which allows 10 digits for the number of effective digits of measurement values.

The data transmission speed differs depending on the long format setting.

### Measurement Value and Judgment Value Formats

### About signs

When a value is negative, a minus "-" sign is added before the measurement value.

When a value is positive, a space " " sign is added before the measurement value.