### Querying measurement data

Syntax | Command |
Query | :MEASure? <no data/ ALL> (ALL can be specified only in continuous measurement mode.)
Response | <Measurement data> (The response format varies depending on the mode.) #### ASCII format <LCR mode> <ANALYZER mode> #### Binary format <LCR mode> <ANALYZER mode>
Parameter |
Explanation | Command |
Query | Returns the status, judgment results, measurement values, and panel number. Set the response content with the :MEASure:VALid command. You can select the type of parameters to return with the :MEASure:ITEM command. For details, refer to the :MEASure:ITEM command. Switching between ASCII mode and binary mode can be set with the :FORMat:DATA command. During continuous measurement, a message terminator or slash (/) is inserted for each single panel measurement. When :MEASure? : Message terminator When :MEASure? ALL : Slash (/)
Example | Command |
Query | :MEASure?
Response | #### ASCII format <LCR mode> <ANALYZER mode> #### Binary format <LCR mode> <ANALYZER mode>
注記 |  | In the query example, the following are set before sending the :MEASure? command. :MEASure:ITEM 0,0,0 :MEASure:VALid 31

### Response(MEASure? or :MEMory?)

##### LCR mode/ANALYZER mode/CONTINUOUS mode