Command | Data | Explanation | L C R | A N A L Y Z E R | C O N T I N U O U S
--- | --- | --- | --- | --- | ---
## Common Commands
*CLS |  | Clearing the status byte register and related queues (except the output queue) |  |  |
*ESE | <Mask value> | Reading and writing the standard event status enable register (SESER) |  |  |
*ESE? |
*ESR? |  | Reading and clearing the standard event status register (SESR) |  |  |
*IDN? |  | Querying the instrument ID (Identification Code) |  |  |
*OPC |  | Setting OPC of SESR after all of the actions being executed are finished |  |  |
*OPC? |  | Sending response of ASCII 1 after all of the actions being executed are finished |  |  |
*RST |  | Initializing the instrument |  |  |
*SRE | <Mask value> | Writing and reading the service request enable register (SRER) |  |  |
*SRE? |
*STB? |  | Reading the Status Byte Register |  |  |
*TRG |  | Requesting a Sample |  |  |
*TST? |  | Executing self tests and querying results |  |  |
*WAI |  | Executing following command after command processing is finished |  |  |
## Event Registers
:ESE0 | <Mask value> | Writing and reading event status enable register 0 |  |  |
:ESE0? |
:ESE1 | <Mask value> | Writing and reading event status enable register 1 |  |  |
:ESE1? |
:ESE2 | <Mask value> | Writing and reading event status enable register 2 |  |  |
:ESE2? |
:ESE3 | <Mask value> | Writing and reading event status enable register 3 |  |  |
:ESE3? |
:ESE4 | <Mask value> | Writing and reading event status enable register 4 |  |  |
:ESE4? |
:ESR0? |  | Reading event status register 0 |  |  |
:ESR1? |  | Reading event status register 1 |  |  |
:ESR2? |  | Reading event status register 2 |  |  |
:ESR3? |  | Reading event status register 3 |  |  |
:ESR4? |  | Reading event status register 4 |  |  |
## Measurement Mode
:MODE | <LCR/ANALyzer/CONTinuous> | Setting and querying measurement mode |  |  |
:MODE? |
## Trigger
:TRIGger | <INTernal/EXTernal> | Setting and querying the trigger mode |  |  |
:TRIGger? |
:TRIGger:DELay | <Trigger delay time> | Setting and querying the trigger delay time |  |  |
:TRIGger:DELay? |
## Parameter Settings
:PARameter# | <Z/ Y/ PHASE(phase angle)/ CS/ CP/ D/ LS/ LP/ Q/ RS/ G/ RP/ X/ B/ OFF> | Setting and querying the display parameters (# is a numerical value from 1 to 4) |  |  |
:PARameter#? |
:PARameter#:DIGit | <Number of display digits> | Setting and querying number of display digits (# is a numerical value from 1 to 4) |  |  |
:PARameter#:DIGit? |
:PARameter:ABSolute | <Z/Y/RS/RP/CS/CP/D/G/X/LS/LP/Q/B>, <ON/OFF> | Setting of the absolute value display and queries |  |  |
:PARameter:ABSolute? | <Z/Y/RS/RP/CS/CP/D/G/X/LS/LP/Q/B>
## Trigger Synchronous Output Function
:SSOurce | <ON/OFF> | Setting and querying the trigger synchronous output function |  |  |
:SSOurce? |
:SSOurce:WAIT | <Wait time> | Setting and querying the wait time of trigger synchronous output |  |  |
:SSOurce:WAIT? |
:SSOurce:INDEX | <Wait time> | Setting of the delay time from when the signal is turned OFF until INDEX is turned ON and queries |  |  |
:SSOurce:INDEX? |
## Measurement Frequency
:FREQuency | LCR mode: <Frequency> Analyzer mode:<Sweep point>,<Frequency> | Setting and querying the Measurement Frequency |  |  |
:FREQuency? | LCR mode: None Analyzer mode:<Sweep point>
## Measurement Signal Level
:LEVel | <P/V/I> | Setting and querying the measurement signal level |  |  |
:LEVel? |
:LEVel:POWer | LCR mode: <power level>/ analyzer mode: <sweep point No.>, <power level> | Setting of the power level value and queries |  |  |
:LEVel:POWer? | LCR mode: none/ analyzer mode: <sweep point No.>
:LEVel:VOLTage | LCR mode: <voltage level>/ analyzer mode: <sweep point No.>, <power level> | Setting of the voltage level value and queries |  |  |
:LEVel:VOLTage? | LCR mode: none/ analyzer mode: <sweep point No.>
:LEVel:CURRent | LCR mode: <current level>/ analyzer mode: <sweep point No.>, <current level> | Setting of the current level value and queries |  |  |
:LEVel:CURRent? | LCR mode: none/ analyzer mode: <sweep point No.>
## Measurement Speed
:SPEEd | LCR mode: <FAST/MEDium/SLOW/SLOW2/CUSTom>/ analyzer mode: <sweep point No.>, <FAST/MEDium/SLOW/SLOW2/CUSTom> | Setting of the measurement speed and queries |  |  |
:SPEEd? | LCR mode: none/ analyzer mode: <sweep point No.>
:SPEEd:WAVE | LCR mode: <number of waveforms>/ analyzer mode: <sweep point No.>, <number of waveforms> | Setting of the measurement speed when the measurement speed is custom and queries |  |  |
:SPEEd:WAVE? |
## Average Function
:AVERaging | LCR mode: <OFF/number of averaging times>/ analyzer mode: <sweep point No.>, <OFF/number of averaging times> | Setting of the measurement average and queries |  |  |
:AVERaging? |
## Judgment Function
:JUDGment | <NORMal/COMParator/BIN> | Setting and querying the judgment function |  |  |
:JUDGment? |
## Comparator Function
:COMParator | <OFF/ON> | Setting and querying ON/ OFF of comparator function |  |  |
:COMParator? |
:COMParator:FLIMit:ABSolute | <OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the MAIN parameter of the comparator function (absolute value mode) |  |  |
:COMParator:FLIMit:ABSolute? |
:COMParator:FLIMit:DEViation | <Reference value>,<OFF/ Lower limit values>,<OFF/ Upper limit values> | Setting and querying the reference value and the upper and lower limit values of the MAIN parameter of the comparator function (deviation percentage (Δ%) mode) |  |  |
:COMParator:FLIMit:DEViation? |
:COMParator:FLIMit:MODE | <ABSolute/PERcent/DEViation> | Setting and querying the judgment mode of the MAIN parameter of the comparator function |  |  |
:COMParator:FLIMit:MODE? |
:COMParator:FLIMit:PERcent | <Reference value>,<OFF/ Lower limit values>,<OFF/ Upper limit values> | Setting and querying the reference value and the upper and lower limit values of the MAIN parameter of the comparator function (percentage (%) mode) |  |  |
:COMParator:FLIMit:PERcent? |
:COMParator:SLIMit:ABSolute | <OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the SUB parameter of the comparator function (absolute value mode) |  |  |
:COMParator:SLIMit:ABSolute? |
:COMParator:SLIMit:DEViation | <Reference value>,<OFF/ Lower limit values>,<OFF/ Upper limit values> | Setting and querying the reference value and the upper and lower limit values of the SUB parameter of the comparator function (deviation percentage (Δ%) mode) |  |  |
:COMParator:SLIMit:DEViation? |
:COMParator:SLIMit:MODE | <ABSolute/PERcent/DEViation> | Setting and querying the judgment mode of the SUB parameter of the comparator function |  |  |
:COMParator:SLIMit:MODE? |
:COMParator:SLIMit:PERcent | <Reference value>,<OFF/ Lower limit values>,<OFF/ Upper limit values> | Setting and querying the reference value and the upper and lower limit values of the SUB parameter of the comparator function (percentage mode) |  |  |
:COMParator:SLIMit:PERcent? |
:COMParator:ABSolute | <Parameter number>, <OFF/lower limit value>, <OFF/upper limit value> | Setting of the upper and lower limit values of the comparator function and queries (absolute mode) |  |  |
:COMParator:ABSolute? | <Parameter number>
:COMParator:DEViation | <Parameter number>, <reference value>, <OFF/lower limit value>, <OFF/upper limit value> | Setting of the reference, upper, and lower limit values of the comparator function (deviation percentage (Δ%) mode) and queries |  |  |
:COMParator:DEViation? | <Parameter number>
:COMParator:MODE | <Parameter number>, <ABSolute/PERcent/DEViation> | Setting of the judgment mode for the comparator function and queries |  |  |
:COMParator:MODE? | <Parameter number>
:COMParator:PERcent | <Parameter number>, <reference value>, <OFF/lower limit value>, <OFF/upper limit value> | Setting of the reference, upper, and lower limit values of the comparator function (percentage (%) mode) and queries |  |  |
:COMParator:PERcent? | <Parameter number>
:COMParator:JUDGment | <DO/NOT> | Setting of the judgment procedure when the measured value of the comparator function is outside the guaranteed accuracy and queries |  |  |
:COMParator:JUDGment? |
## BIN Function
:BIN | <OFF/ON> | Setting and querying ON/ OFF of BIN function |  |  |
:BIN? |
:BIN:FLIMit:ABSolute | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the MAIN parameter of the BIN function (absolute value mode) |  |  |
:BIN:FLIMit:ABSolute? | <BIN number>
:BIN:FLIMit:DEViation | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the MAIN parameter of the BIN function (deviation percentage (Δ%) mode) |  |  |
:BIN:FLIMit:DEViation? | <BIN number>
:BIN:FLIMit:MODE | <ABSolute/PERcent/DEViation> | Selecting and querying the mode of the MAIN parameter of the BIN function |  |  |
:BIN:FLIMit:MODE? |
:BIN:FLIMit:PERcent | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the MAIN parameter of the BIN function (percentage (%) mode) |  |  |
:BIN:FLIMit:PERcent? | <BIN number>
:BIN:FLIMit:REFerence | <Reference value> | Setting and querying the reference value of the MAIN parameter of the BIN function (percentage (%) mode and deviation percentage (Δ%) mode) |  |  |
:BIN:FLIMit:REFerence? |
:BIN:SLIMit:ABSolute | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the SUB parameter of the BIN function (absolute value mode) |  |  |
:BIN:SLIMit:ABSolute? | <BIN number>
:BIN:SLIMit:DEViation | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the SUB parameter of the BIN function (deviation percentage (Δ%) mode) |  |  |
:BIN:SLIMit:DEViation? | <BIN number>
:BIN:SLIMit:MODE | <ABSolute/PERcent/DEViation> | Selecting and querying the mode of the SUB parameter of the BIN function |  |  |
:BIN:SLIMit:MODE? |
:BIN:SLIMit:PERcent | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the SUB parameter of the BIN function (percentage (%) mode) |  |  |
:BIN:SLIMit:PERcent? | <BIN number>
:BIN:SLIMit:REFerence | <Reference value> | Setting and querying the reference value of the SUB parameter of the BIN function (percentage (%) mode and deviation percentage (Δ%) mode) |  |  |
:BIN:SLIMit:REFerence? |
:BIN:ABSolute | <Parameter number>, <BIN number>, <OFF/lower limit value>, <OFF/upper limit value> | Setting of the upper and lower limit values of the BIN function and queries (absolute mode) |  |  |
:BIN:ABSolute? | <Parameter number>, <BIN number>
:BIN:DEViation | <Parameter number>, <BIN number>, <OFF/lower limit value>, <OFF/upper limit value> | Setting of the upper and lower limit values of the BIN function (deviation percentage (Δ%) mode) and queries |  |  |
:BIN:DEViation? | <Parameter number>, <BIN number>
:BIN:MODE | <Parameter number>, <ABSolute/PERcent/DEViation> | Setting of the judgment mode for the BIN function and queries |  |  |
:BIN:MODE? | <Parameter number>
:BIN:PERcent | <Parameter number>, <BIN number>, <OFF/lower limit value>, <OFF/upper limit value> | Setting of the upper and lower limit values of the BIN function (percentage (%) mode) and queries |  |  |
:BIN:PERcent? | <Parameter number>, <BIN number>
:BIN:REFerence | <Parameter number>, <reference value> | Setting of the reference value of the BIN function (percentage (%) mode and deviation percentage (Δ%) mode) and queries |  |  |
:BIN:REFerence? | <Parameter number>
## Measurement Value Output
:MEASure? |  | Querying measurement data |  |  |
:MEASure:RDC? |  | Queries for the contact check measurement data |  |  |
## Sweep Method Settings
:SWEep:MAIN:SOURce | <FREQuency/POWer/V/I> | Setting and querying main sweep measurement signal mode |  |  |
:SWEep:MAIN:SOURce? |
:SWEep:PDELay | <Sweep point No.>, <point delay time> | Setting of the point delay and queries |  |  |
:SWEep:PDELay? | <Sweep point No.>
:SWEep:TRIGger | <SEQuential/REPeat/STEP> | Setting and querying trigger mode |  |  |
:SWEep:TRIGger? |
:SWEep:DISPlay | <GRAPh/FGRAPh/XY/XY2/MULTi/NUMEric/PEAK> | Setting of the display for the analyzer mode and queries |  |  |
:SWEep:DISPlay? |
## Sweep Point Settings
:POINt | <Sweep point No.>,<Setting value> | Setting and querying the sweep point |  |  |
:POINt? | <Sweep point No.>
:POINt:ADD | <Sweep point No.>, <set value> | Adding a sweep point |  |  |
:POINt:DELete | <Sweep point No.> | Deletion of sweep point |  |  |
## Sweep Point List Settings
:LIST:STARt:STOP | <START value>,<STOP value>,<Number of sweep points>,<LINear/ LOG> | Setting and querying the sweep point settings of START-STOP mode |  |  |
:LIST:STARt:STOP? |
:LIST:STARt:STEP | <START value>,<STEP value>,<Number of sweep points> | Setting and querying the sweep point settings of START-STEP mode |  |  |
:LIST:STARt:STEP? |
:LIST:CENTerspan | <CENTER value>,<SPAN value>,<Number of sweep points> | Simultaneously setting and querying sweep point settings of the CENTER-SPAN method |  |  |
:LIST:CENTerspan? |
:LIST:INTerval | <POINT value>,<INTERVAL value>,<Number of sweep points> | Setting and querying the sweep point settings of INTERVAL mode |  |  |
:LIST:INTerval? |
## Segment Function
:SEGMent | <ON/OFF/INTerval> | Setting of the segment function and queries |  |  |
:SEGMent? |
:SEGMent:ADD | <Segment No./ no data> | Adding a segment |  |  |
:SEGMent:DELete | <Segment No.> | Deleting the specified segment |  |  |
:SEGMent:NUM? |  | Querying the number of segments |  |  |
:SEGMent:AVERaging | <Segment No.>, <OFF/number of averaging times> | Setting of the number of averaging times for the specified segment and queries |  |  |
:SEGMent:AVERaging? | <Segment No.>
:SEGMent:PDELay | <Segment No.>,<Delay time> | Setting and querying the point delay time of the specified segment |  |  |
:SEGMent:PDELay? | <Segment No.>
:SEGMent:SPEEd | <Segment No.>,<FAST/MEDium/SLOW/SLOW2> | Setting and querying the measurement speed of the specified segment |  |  |
:SEGMent:SPEEd? | <Segment No.>
:SEGMent:SPEEd:WAVE | <Segment No.>, <number of waveforms> | Setting of the measurement speed when the measurement speed is custom for the specified segment and queries |  |  |
:SEGMent:SPEEd:WAVE? | <Segment No.>
:SEGMent:SUB:SOURce | <P/V/I> | Setting and querying measurement signal for when segment sweep |  |  |
:SEGMent:SUB:SOURce? |
:SEGMent:SUB:SOURce:VALue | <Segment No.>,<Signal source value> | Setting and querying the measurement signal level of the specified segment |  |  |
:SEGMent:SUB:SOURce:VALue? | <Segment No.>
:SEGMent:STARt:STOP | <Segment No.>,<START value>,<STOP value>,<Number of sweep points>, <LINear/LOG> | Simultaneously setting and querying sweep point settings of START-STOP method of specified segment |  |  |
:SEGMent:STARt:STOP? | <Segment No.>
:SEGMent:INTerval | <Segment No.>, <POINT value>, <interval time>, <Number of sweep points> | Setting of the interval time of the specified segment and queries |  |  |
:SEGMent:INTerval? | <Segment No.>
## Graph Display
:GRAPh:AUTOscale |  | Executing auto scaling |  |  |
:GRAPh:COLor | <Segment No.>, <parameter number>, <OFF/color No.> | Setting of the graph display color and queries |  |  |
:GRAPh:COLor? | <Segment No.>, <parameter number>
:GRAPh:COLor:RESet | <Parameter No.> | Executing reset of the graph display colors of all segments |  |  |
:GRAPh:COLor:SEG1 | <Parameter No.> | Reflecting the display color of segment 1 to all segments |  |  |
:GRAPh:OVERwrite | <ON/OFF> | Setting and querying the overwrite function |  |  |
:GRAPh:OVERwrite? |
:GRAPh:OVERwrite:CLEar |  | Clearing of overdrawing |  |  |
:GRAPh:SCALe | <LINear/LOG> | Setting and querying the horizontal axis display scale |  |  |
:GRAPh:SCALe? |
:GRAPh:SPAN | <SINGle/SEGMent> | Setting and querying the horizontal axis span format |  |  |
:GRAPh:SPAN? |
:GRAPh:VERTical:CENTerdiv | <Parameter No.>,<Reference value>,<One graduation width> | Setting and querying the reference value and graduation width of the vertical axis display scale |  |  |
:GRAPh:VERTical:CENTerdiv? | <Parameter No.>
:GRAPh:VERTical:GRID | <Graph No.>, <Parameter No.> | Setting and querying the parameters to display grid |  |  |
:GRAPh:VERTical:GRID? | <Graph No.>
:GRAPh:VERTical:METHod | <Parameter No.>, <UPPer/CENTer> | Setting and querying the setting method for the vertical axis display scale |  |  |
:GRAPh:VERTical:METHod? | <Parameter No.>
:GRAPh:VERTical:MODE | <Parameter No.>, <AUTO/MANual> | Setting and querying the vertical axis display scale method |  |  |
:GRAPh:VERTical:MODE? | <Parameter No.>
:GRAPh:VERTical:REVerse | <Graph No.>, <OFF/ON> | Setting and querying the reversing of the display scale along the vertical axis |  |  |
:GRAPh:VERTical:REVerse? | <Graph No.>
:GRAPh:VERTical:SCALe | <Parameter No.>, <LINear/LOG> | Setting and querying the vertical axis display scale |  |  |
:GRAPh:VERTical:SCALe? | <Parameter No.>
:GRAPh:VERTical:UPPerlower | <Parameter No.>,<Lower limit values>,<Upper limit values> | Setting and querying the upper and lower limit values of the vertical axis display scale |  |  |
:GRAPh:VERTical:UPPerlower? | <Parameter No.>
:GRAPh:VERTical:XYGRaph | <INDividual/SAME> | Setting and querying the scaling method during automatic scaling for the X-Y display |  |  |
:GRAPh:VERTical:XYGRaph? |
## Display Cursor
:CURSor | <OFF/A/AB> | Setting and querying the display cursor setting |  |  |
:CURSor? |
:CURSor:#SEARch | <MAX/MIN/TARGet/LMAX/LMIN> | Setting and querying the search method (# is A or B) |  |  |
:CURSor:#SEARch? |
:CURSor:#SEARch:PARameter | <Parameter No.> | Setting and querying the search parameter (# is A or B) |  |  |
:CURSor:#SEARch:PARameter? |
:CURSor:#SEARch:TARGet | <TARGET value> | Setting and querying the target value (# is A or B) |  |  |
:CURSor:#SEARch:TARGet? |
:CURSor:#SEARch:TARGet:SLOPe | <UP/DOWN> | Setting of the target slope and queries (# indicates A or B) |  |  |
:CURSor:#SEARch:TARGet:SLOPe? |
:CURSor:MOVE | <A/B> | Setting and querying the cursor to move or perform searches. |  |  |
:CURSor:MOVE? |
:CURSor:SEARch:AUTO | <ON/OFF> | Setting and querying the auto search |  |  |
:CURSor:SEARch:AUTO? |
## Search Function
:SEARch |  | Executing the search function |  |  |
:SEARch? | <A/B>
## Comparator Function
:COMParator:ANALyzer | <OFF/AREA/PEAK> | Setting and querying comparator judgment mode |  |  |
:COMParator:ANALyzer? |
:COMParator:AREA | <Graph No.>, <OFF/1/2/3/4> | Setting and querying drawing of judgment area |  |  |
:COMParator:AREA? | <Graph No.>
:COMParator:AREA:FIX | <Segment No.>,<Parameter No.>,<PERcent/VALue>,<Reference value>,<Lower limit values>,<Upper limit values> | Setting and querying area judgment (reference value manual setting) |  |  |
:COMParator:AREA:FIX? | <Segment No.>,<Parameter No.>
:COMParator:AREA:LIMit | <Sweep point No.>,<Parameter No.>,<Lower limit values>,<Upper limit values> | Setting and querying the upper and lower limit values for area judgment |  |  |
:COMParator:AREA:LIMit? | <Sweep point No.>,<Parameter No.>
:COMParator:AREA:MEAS | <Segment No.>,<Parameter No.>,<PERcent/ VALue>,<Lower limit values>,<Upper limit values> | Setting and querying area judgment (reference value automatic setting) |  |  |
:COMParator:AREA:MEAS? | <Segment No.>,<Parameter No.>
:COMParator:PARAmeter | <Parameter No./ALL>, <ON/OFF> | Setting and querying judgment parameter |  |  |
:COMParator:PARAmeter? | <Parameter No.>
:COMParator:PEAK | <Segment No.>,<Parameter No.>,<MAX/MIN>,<OFF/Left limit value>,<OFF/Right limit value>,<OFF/Lower limit values>,<OFF/Upper limit values> | Setting and querying peak judgment |  |  |
:COMParator:PEAK? | <Segment No.>,<Parameter No.>,<MAX/MIN>
:COMParator:PEAK:FILTer | <ON/OFF> | Setting and querying the filter value |  |  |
:COMParator:PEAK:FILTer? |
:COMParator:PEAK:NO | <Local minimum No.>, <Local maximum No.> | Setting and querying the local maximum number and local minimum number |  |  |
:COMParator:PEAK:NO? |
## Measurement Value Output
:MEASure? | <No data> | Querying measurement data |  |  |
:MEASure:RDC? |  | Queries for the contact check measurement data |  |  |
:MEASure:COMParator:PEAK? |  | Querying the overall judgment result when peak comparator measurement |  |  |
:MEASure:COMParator:PEAK:LMAX? | <Segment No.>,<Parameter No.> | Querying the judgment result of the local maximum value when peak comparator measurement |  |  |
:MEASure:COMParator:PEAK:LMIN? | <Segment No.>,<Parameter No.> | Querying the judgment result of the local minimum value when peak comparator measurement |  |  |
:MEASure:CURSor? | <A/B> | Querying the measurement data of the cursor position |  |  |
:MEASure:POINt? | <Sweep point> | Querying the measurement data of the specified sweep point |  |  |
## Equivalent circuit analysis function
:CIRCuit:ANALysis | <OFF/HOLD/AUTO> | Setting of the equivalent circuit analysis function and queries |  |  |
:CIRCuit:ANALysis? |
:CIRCuit:ANALysis:FREQuency | <Analysis start frequency>, <analysis end frequency> | Setting of the frequency range of the equivalent circuit analysis and queries |  |  |
:CIRCuit:ANALysis:FREQuency? |
:CIRCuit:ANALysis:K:MODE | <KR/K31/K33/KT/K15> | Setting and querying the vibration mode for calculation of the coupling coefficient (K) of an electric machine |  |  |
:CIRCuit:ANALysis:K:MODE? |
:CIRCuit:ANALysis:K:TYPE | <FSFP/FRFA> | Setting and querying the frequency type for calculation of the coupling coefficient (K) of an electric machine |  |  |
:CIRCuit:ANALysis:K:TYPE? |
:CIRCuit:ANALysis:K:COEFficient | <Coefficient a>, <Coefficient b> | Setting and querying the coefficient for calculation of the coupling coefficient (K) of an electric machine |  |  |
:CIRCuit:ANALysis:K:COEFficient? |
:CIRCuit:ANALysis:MODel | <A/B/C/D/E> | Setting of the equivalent circuit model and queries |  |  |
:CIRCuit:ANALysis:MODel? |
:CIRCuit:ANALysis:RESult? | <R1/C1/L1/C0/QM/K> | Queries of the R1, C1, L1, and C0 values. |  |  |
:CIRCuit:ANALysis:RESult:POSition | <UL/UR/LL/LR> | Setting of the display position of the analysis result and queries |  |  |
:CIRCuit:ANALysis:RESult:POSition? |
:CIRCuit:ANALysis:SEGMent | <Segment No./ALL> | Setting of the equivalent circuit analysis segment range and queries |  |  |
:CIRCuit:ANALysis:SEGMent? |
:CIRCuit:ANALysis:SIMulation |  | Execution of frequency characteristics simulation |  |  |
:CIRCuit:ANALysis:SIMulation:GET |  | Execution of frequency characteristics simulation |  |  |
:CIRCuit:ANALysis:SIMulation:DEFine | <R1/C1/L1/C0>, <Constant> | Setting of frequency characteristics simulation and queries |  |  |
:CIRCuit:ANALysis:SIMulation:DEFine? | <R1/C1/L1/C0>
:CIRCuit:ANALysis:TRIGger |  | Executes the equivalent circuit analysis. |  |  |
:CIRCuit:ANALysis:TRIGger:AUTO | <ON/OFF> | Setting of the automatic equivalent circuit analysis and queries |  |  |
:CIRCuit:ANALysis:TRIGger:AUTO? |
:COMParator:CIRCuit:ANALysis | <ON/OFF> | Comparator function on/off setting for analysis results and inquiry |  |  |
:COMParator:CIRCuit:ANALysis? |
:COMParator:CIRCuit:ANALysis:ABSolute | <L1/C1/R1/QM/C0>, <Off/lower limit value>, <Off/upper limit value> | Comparator upper and lower value settings for analysis results and inquiry |  |  |
:COMParator:CIRCuit:ANALysis:ABSolute? | <L1/C1/R1/QM/C0>
:MEASure:ANALysis:COMParator? |  | Comparator judgment results for analysis results inquiry |  |  |
:MEASure:ANALysis:DELTa? |  | Difference between measured value and simulation value inquiry |  |  |
:MEASure:ANALysis:PEAK? | <Z/G/B/RS>, <LMAX/LMIN> | Acquisition of local extreme value frequency and measured values (models A to E only) |  |  |
:MEASure:ANALysis:SIMulation? | <Parameter No.> | Simulation value inquiry |  |  |
## Calibration and compensation function (common setting)
:CORRection:FORMat:OPEN | <Display method> | Setting of the display method of the open calibration and compensation and queries |  |  |
:CORRection:FORMat:OPEN? |
:CORRection:FORMat:SHORt | <Display method> | Setting of the display method of the short calibration and compensation and queries |  |  |
:CORRection:FORMat:SHORt? |
:CORRection:FORMat:LOAD | <Display method> | Setting of the display method of the load calibration and compensation and queries |  |  |
:CORRection:FORMat:LOAD? |
:CORRection:LIMit:POINt | <Compensation minimum frequency>, <Compensation maximum frequency> | Setting of the frequency range of the ALL calibration and compensation and queries |  |  |
:CORRection:LIMit:POINt? |
:CORRection:DISTance | <Electrical length> | Setting of the electrical length for calibration and compensation and queries |  |  |
:CORRection:DISTance? |
:CORRection:ERRor? |  | Queries for the calibration and compensation execution result |  |  |
## Calibration function
:CORRection:CALIbration:RETurn | LCR mode: <OFF/ALL/SPOT> / Analyzer mode: <OFF/SPOT> | Setting of the calibration and queries |  |  |
:CORRection:CALIbration:RETurn? |
:CORRection:CALIbration:RESet | <Calibration No./ALL/DC>, <DATA/REFerence> | Calibration resetting |  |  |
:CORRection:CALIbration:FREQuency | <Calibration No.>, <frequency/OFF> | Setting of the frequency for the calibration point and queries |  |  |
:CORRection:CALIbration:FREQuency? | <Calibration No.>
:CORRection:CALIbration:LEVel | <P/V/I>, <Calibration No./ALL>, <level value/OFF> | Setting of the level value for the calibration point and queries |  |  |
:CORRection:CALIbration:LEVel? | <P/V/I>, <Calibration No.>
:CORRection:CALIbration:SPEEd | SPOT calibration: <calibration No./ALL>, <FAST/MEDium/SLOW/SLOW2/CUSTom>, ALL calibration: <FAST/MEDium/SLOW/SLOW2/CUSTom> | Setting of the calibration point speed and queries |  |  |
:CORRection:CALIbration:SPEEd? | SPOT calibration: <calibration No.>/ ALL calibration: none
:CORRection:CALIbration:WAVE | SPOT calibration: <calibration No./ALL>, <number of waveforms>, ALL calibration: <number of waveforms> | Setting of the number of waveforms for the calibration point and queries |  |  |
:CORRection:CALIbration:WAVE? | SPOT calibration: <calibration No.>/ ALL calibration: none
:CORRection:CALIbration:OPEN | <AC/DC/ACDC/CANCel> | Execution and cancellation of open calibration |  |  |
:CORRection:CALIbration:OPEN:REFerence | <Calibration No./ALL/DC>, <reference value 1>, <reference value 2 *disabled for DC> | Setting of the reference value for open calibration and queries |  |  |
:CORRection:CALIbration:OPEN:REFerence? | <Calibration No./DC>
:CORRection:CALIbration:OPEN:DATA? | SPOT compensation: <compensation No./DC>/ ALL compensation: <compensation No./ALL/DC> | Queries for the calibration value for open calibration |  |  |
:CORRection:CALIbration:OPEN:LIMit | <OFF/lower limit value> | Setting of the lower limit value for open calibration and queries |  |  |
:CORRection:CALIbration:OPEN:LIMit? |
:CORRection:CALIbration:SHORt | <AC/DC/ACDC/CANCel> | Execution and cancellation of short calibration |  |  |
:CORRection:CALIbration:SHORt:REFerence | <Calibration No./ALL/DC>, <reference value 1>, <reference value 2 *disabled for DC> | Setting of the reference value for short calibration and queries |  |  |
:CORRection:CALIbration:SHORt:REFerence? | <Calibration No./DC>
:CORRection:CALIbration:SHORt:DATA? | SPOT compensation: <compensation No./DC>/ ALL compensation: <compensation No./ALL/DC> | Queries for the short calibration value |  |  |
:CORRection:CALIbration:SHORt:LIMit | <OFF/upper limit value> | Setting of the upper limit value for short calibration and queries |  |  |
:CORRection:CALIbration:SHORt:LIMit? |
:CORRection:CALIbration:LOAD | <AC/DC/ACDC/CANCel> | Execution and cancellation of load calibration |  |  |
:CORRection:CALIbration:LOAD:REFerence | <Calibration No./ALL/DC>, <reference value 1>, <reference value 2 *disabled for DC> | Setting of the reference value for load calibration and queries |  |  |
:CORRection:CALIbration:LOAD:REFerence? | <Calibration No./DC>
:CORRection:CALIbration:LOAD:DATA? | SPOT compensation: <compensation No./DC>/ ALL compensation: <compensation No./ALL/DC> | Queries for the load calibration value |  |  |
:CORRection:CALIbration:LOAD:LIMit | <OFF/lower limit value>, <OFF/upper limit value> | Setting of the upper and lower limit values for load calibration and queries |  |  |
:CORRection:CALIbration:LOAD:LIMit? |
## Compensation function
:CORRection:COMPensation:RETurn | <OFF/ON> | Setting of compensation and queries |  |  |
:CORRection:COMPensation:RETurn? |
:CORRection:COMPensation:RESet | <Compensation No./ALL/DC>, <DATA/REFerence> | Compensation resetting |  |  |
:CORRection:COMPensation:FREQuency? | <Compensation No.> | Queries for the frequency for the compensation point |  |  |
:CORRection:COMPensation:LEVel? | <P/V/I>, <Compensation No.> | Queries for the level value for the compensation point |  |  |
:CORRection:COMPensation:SPEEd? | SPOT compensation: <compensation No.>/ ALL compensation: none | Queries for the compensation point speed |  |  |
:CORRection:COMPensation:WAVE |  | Queries for the number of waveforms for the compensation point |  |  |
:CORRection:COMPensation:WAVE? | SPOT compensation: <compensation No.>/ ALL compensation: none
:CORRection:COMPensation:OPEN | <AC/DC/ACDC/CANCel> | Execution and cancellation of open compensation |  |  |
:CORRection:COMPensation:OPEN:REFerence | <Compensation No./ALL/DC>, <reference value 1>, <reference value 2 *disabled for DC> | Setting of the reference value for open compensation and queries |  |  |
:CORRection:COMPensation:OPEN:REFerence? | <Compensation No./DC>
:CORRection:COMPensation:OPEN:DATA? | SPOT compensation: <compensation No./DC>/ ALL compensation: <compensation No./ALL/DC> | Queries for the compensation value for open compensation |  |  |
:CORRection:COMPensation:OPEN:LIMit | <OFF/lower limit value> | Setting of the lower limit value for open compensation and queries |  |  |
:CORRection:COMPensation:OPEN:LIMit? |
:CORRection:COMPensation:SHORt | <AC/DC/ACDC/CANCel> | Execution and cancellation of short compensation |  |  |
:CORRection:COMPensation:SHORt:REFerence | <Compensation No./ALL/DC>, <reference value 1>, <reference value 2 *disabled for DC> | Setting of the reference value for short compensation and queries |  |  |
:CORRection:COMPensation:SHORt:REFerence? | <Compensation No./DC>
:CORRection:COMPensation:SHORt:DATA? | SPOT compensation: <compensation No./DC>/ ALL compensation: <compensation No./ALL/DC> | Queries for the reference value for short compensation |  |  |
:CORRection:COMPensation:SHORt:LIMit | <OFF/upper limit value> | Setting of the upper limit value for short compensation and queries |  |  |
:CORRection:COMPensation:SHORt:LIMit? |
## Scaling compensation function
:CORRection:SCALe | <OFF/ON> | Setting of the scaling compensation function and queries |  |  |
:CORRection:SCALe? |
:CORRection:SCALe:DATA | <Scale No.>, <compensation value A>, <compensation value B> | Setting of the scaling compensation value and queries |  |  |
:CORRection:SCALe:DATA? | <Scale No.>
## Continuous measurement settings
:CONTinuous:EXECution | <Panel No.>, <ON/OFF> | Setting and querying the continuous measurement target |  |  |
:CONTinuous:EXECution? | <Panel No.>
:CONTinuous:ERRor | <ON/OFF> | Setting of the finish function for a judgment error and queries |  |  |
:CONTinuous:ERRor? |
:CONTinuous:COUNt? |  | Panel count targeted for measurement in continuous measurement mode inquiry |  |  |
## Measurement Value Output
:MEASure? | <No data/ ALL> | Querying measurement data |  |  |
:MEASure:RDC? |  | Queries for the contact check measurement data |  |  |
:MEASure:CONTinuous:COMParator? |  | Querying the overall judgment result when continuous measurement |  |  |
:MEASure:CONTinuous:PEAK? | <No data/ ALL> | Querying the judgment results of the extreme values when continuous measurement |  |  |
## Contact Check Function
:CCHeck:VERify | <OFF/BEFore/AFTer/BOTH> | Setting and querying the contact check function |  |  |
:CCHeck:VERify? |
:CCHeck:JUDGment | <DO/NOT> | Setting of whether a judgment is performed/not performed when the DC measured value is UNCAL for the contact check function and queries |  |  |
:CCHeck:JUDGment? |
:CCHeck:WAVe | <Number of waveforms> | Setting of the contact check execution time and queries |  |  |
:CCHeck:WAVe? |
:CCHeck:LIMit | <OFF/lower limit value>, <OFF/upper limit value> | Setting of the upper and lower limit values for the contact check judgment condition and queries |  |  |
:CCHeck:LIMit? |
:CCHeck:ERREnd | <OFF/ON> | Setting of the measurement stop for a contact check error and queries |  |  |
:CCHeck:ERREnd? |
:CCHeck:ACOut | <OFF/ON> | Setting of the AC output during contact check and queries |  |  |
:CCHeck:ACOut? |
:CCHeck:DCWait | <Wait time> | Setting of the DC wait time during contact check and queries |  |  |
:CCHeck:DCWait? |
:CCHeck:ACWait | <Wait time> | Setting of the AC wait time during contact check and queries |  |  |
:CCHeck:ACWait? |
:LEVCheck | <ON/OFF> | Setting of the detection level monitoring function for contact check and queries |  |  |
:LEVCheck? |
:LEVCheck:LIMit | <Limit value> | Setting of the limit value for contact check and queries |  |  |
:LEVCheck:LIMit? |
## HIGH- Z reject function
:HIZ | <ON/OFF> | Setting and querying the Hi Z reject function |  |  |
:HIZ? |
:HIZ:LIMit | <Limit value> | Setting and querying the limit value of the Hi Z reject function |  |  |
:HIZ:LIMit? |
## Measurement Value Memory Function
:MEMory? | <No data/ ALL> | Querying measurement values saved to memory with the measurement value memory function |  |  |
:MEMory:SAVE |  | Saving of measured value memory |  |  |
:MEMory:CLEar |  | Clearing memory of measurement value memory function |  |  |
:MEMory:CONTrol | LCR mode:<ON/IN/OFF> / Analyzer mode:<ON/OFF> | Setting and querying the measurement value memory function |  |  |
:MEMory:CONTrol? |
:MEMory:COUNt? |  | Querying the number of measurement values saved to memory with the memory function |  |  |
:MEMory:POINts | <Memory size> | Setting and querying the measurement value memory size |  |  |
:MEMory:POINts? |
## Display Function
:DISPlay | <ON/OFF> | Setting and querying LCD display |  |  |
:DISPlay? |
:DISPlay:PARAmeter | <Parameter number>, <OFF/color No.> | Setting of the parameter color and queries |  |  |
:DISPlay:PARAmeter? | <Parameter number>
:DISPlay:COLor | <WHITe/BLACk> | Setting of the screen background and queries |  |  |
:DISPlay:COLor? |
:DISPlay:BACKlight | <Brightness> | Setting of the screen brightness and queries |  |  |
:DISPlay:BACKlight? |
:DISPlay:WARMup | <ON/OFF> | Setting of the warm-up message display and queries |  |  |
:DISPlay:WARMup? |
## Zoom Function
:ZOOM | <ON/OFF> | Setting and querying the zoom function |  |  |
:ZOOM? |
## Beep Tone
:BEEPer:JUDGment | <OFF/IN/NG> | Setting and querying beep sound for the judgment results of measurement values |  |  |
:BEEPer:JUDGment? |
:BEEPer:JUDGment:TONE | <0/1/2/3/4/5/6/7/8/9/10/11/12/13/14> | Setting of the beep tone type for the measured value judgment result and queries |  |  |
:BEEPer:JUDGment:TONE? |
:BEEPer:JUDGment:VOLume | <1/2/3> | Setting of the beep volume for the measured value judgment result and queries |  |  |
:BEEPer:JUDGment:VOLume? |
:BEEPer:KEY | <ON/OFF> | Setting and querying beep sound for key input |  |  |
:BEEPer:KEY? |
:BEEPer:KEY:TONE | <0/1/2/3/4/5/6/7/8/9/10/11/12/13/14> | Setting of the key operation beep tone type and queries |  |  |
:BEEPer:KEY:TONE? |
:BEEPer:KEY:VOLume | <1/2/3> | Setting of the key operation beep volume and queries |  |  |
:BEEPer:KEY:VOLume? |
## Key Lock
:KEYLock | LCR mode: <FULL/SET> / Analyzer mode: <ON> | Execution of the key lock and queries |  |  |
:KEYLock? |
:KEYLock:PASScode | <Passcode/ none> | Setting the key lock passcode |  |  |
:KEYLock:UNLock | <Passcode/ none> | Disabling the key lock |  |  |
## Measurement Value Output Set
:MEASure:ITEM | <MR0>, <MR1> | Setting and querying measurement parameters |  |  |
:MEASure:ITEM? |
:MEASure:VALid | <Setting value> | Setting and querying the response data of the measurement acquisition query |  |  |
:MEASure:VALid? |
:MEASure:OUTPut:AUTO | <ON/OFF> | Setting and querying the measurement value automatic output function |  |  |
:MEASure:OUTPut:AUTO? |
## EXT I/O Output
:IO:EOM:MODE | <HOLD/PULSe> | INDEX and EMO output method setting and inquiry |  |  |
:IO:EOM:MODE? |
:IO:EOM:PULSe | <Pulse width> | Pulse width for which to keep EOM low (on) setting and inquiry |  |  |
:IO:EOM:PULSe? |
:IO:OUTPut:DELay | <I/O delay time> | Setting and querying the delay time between judgment result output and EOM output |  |  |
:IO:OUTPut:DELay? |
:IO:RESult:RESet | <ON/OFF> | Setting and querying output of the judgment result signal line |  |  |
:IO:RESult:RESet? |
:IO:TRIGger:EDGe | <DOWN/UP> | Setting and querying the trigger edge |  |  |
:IO:TRIGger:EDGe? |
:IO:TRIGger:ENABle | <ON/OFF> | Setting and querying permit/prohibit of trigger input during measurement |  |  |
:IO:TRIGger:ENABle? |
## Panel Save Function
:SAVE | <Panel No.>,<"Panel name"> | Executing and querying the panel save function |  |  |
:SAVE? | <Panel No.>
:SAVE:NAME? | <Panel No.> | Querying a panel name |  |  |
:SAVE:REName | <Panel No.>,<"Panel name"> | Changing a panel name |  |  |
:SAVE:TYPE | <ALL/HARDware/ADJust> | Setting and querying the save type |  |  |
:SAVE:TYPE? |
:SAVE:CLEar | <Panel No./ALL> | Clearing data saved for a panel |  |  |
## Panel Load Function
:LOAD | <Panel No.> | Executing panel load |  |  |
## Message Terminator
:TRANsmit:TERMinator | <Terminator number> | Setting and querying the terminator of the response message |  |  |
:TRANsmit:TERMinator? |
## RS-232C Communication Handshake
:HANDshake | <OFF/X> | Setting and querying the RS-232C Communication Handshake |  |  |
:HANDshake? |
## Data transfer format
:FORMat:DATA | <ASCii/REAL> | Setting and querying the data transfer format |  |  |
:FORMat:DATA? |
:FORMat:LONG | <ON/OFF> | Setting and querying long format for when data transfer |  |  |
:FORMat:LONG? |
## Header
:HEADer | <ON/OFF> | Setting and querying existence of header in response message |  |  |
:HEADer? |
## System Settings
:SYSTem:DATE | <Year>,<Month>,<Day> | Setting and querying the date |  |  |
:SYSTem:DATE? |
:SYSTem:MACAddress? |  | Querying the MAC address |  |  |
:SYSTem:SERIAlno? |  | Querying the serial number |  |  |
:SYSTem:TIME | <Hour>,<Minute>,<Second> | Setting and querying the time |  |  |
:SYSTem:TIME? |
:SYSTem:USBId? |  | Returns the USB ID. |  |  |
:SYSTem:RESet |  | Execution of system resetting |  |  |
## Initialize Device
:PRESet |  | Initializing the instrument |  |  |
## File storage function
:FILE:SAVE |  | Executing file saving |  |  |
:FILE:TYPE:BMP | <OFF/COLor/MONochrome> | BMP save settings and inquiry |  |  |
:FILE:TYPE:BMP? |
:FILE:TYPE:TEXT | <OFF/ON> | Text save settings and inquiry |  |  |
:FILE:TYPE:TEXT? |
:FILE:DATE | <ON/OFF> | Setting and querying the date and time for when saving text |  |  |
:FILE:DATE? |
:FILE:DELIMiter | <COMma/TAB/SEMIcolon/SPACE> | Setting and querying the delimiter for when saving text |  |  |
:FILE:DELIMiter? |
:FILE:FOLDer | <"Folder name"> | Setting and querying the save folder |  |  |
:FILE:FOLDer? |
:FILE:INFOrmation? |  | Querying USB flash drive information |  |  |
:FILE:MODE | <AUTO/MANUAL> | Setting and querying the mode of the save folder |  |  |
:FILE:MODE? |
:FILE:PARAmeter | <ON/OFF> | Setting and querying the measurement parameter setting for when saving text |  |  |
:FILE:PARAmeter? |
:FILE:QUOTe | <OFF/DOUBle/SINGle> | Setting and querying the quotation mark setting for when saving text |  |  |
:FILE:QUOTe? |
:FILE:SET | <ON/OFF> | Setting and querying the measurement condition setting for when saving text |  |  |
:FILE:SET? |
:FILE:PANel:SAVE | <"File name"> | Execution of settings save to USB memory |  |  |
:FILE:PANel:LOAD | <"File name"> | Execution of settings load from USB memory |  |  |
:FILE:PANel:ALLSave | <"Specified save file name"> | Execution of all save to USB memory |  |  |
:FILE:PANel:ALLLoad | <"Specified save file name"> | Execution of all load from USB memory |  |  |
## Monitor Function
:MONItor? |  | Querying the voltage/current monitor value |  |  |
## Screen storage function
:HCOPy:DATA? | <COLor/MONochrome> | Acquiring the BMP data of the measurement screen |  |  |