Command | Data | Explanation | L C R | C O N T I N U O U S
--- | --- | --- | --- | ---
## Common Commands
*CLS |  | Clearing the status byte register and related queues (except the output queue) |  |
*ESE | <Mask value> | Reading and writing the standard event status enable register (SESER) |  |
*ESE? |
*ESR? |  | Reading and clearing the standard event status register (SESR) |  |
*IDN? |  | Querying the instrument ID (Identification Code) |  |
*OPC |  | Setting OPC of SESR after all of the actions being executed are finished |  |
*OPC? |  | Sending response of ASCII 1 after all of the actions being executed are finished |  |
*RST |  | Initializing the instrument |  |
*SRE | <Mask value> | Writing and reading the service request enable register (SRER) |  |
*SRE? |
*STB? |  | Reading the Status Byte Register |  |
*TRG |  | Requesting a Sample |  |
*TST? |  | Executing self tests and querying results |  |
*WAI |  | Executing following command after command processing is finished |  |
## Event Registers
:ESE0 | <Mask value> | Writing and reading event status enable register 0 |  |
:ESE0? |
:ESE1 | <Mask value> | Writing and reading event status enable register 1 |  |
:ESE1? |
:ESE2 | <Mask value> | Writing and reading event status enable register 2 |  |
:ESE2? |
:ESE3 | <Mask value> | Writing and reading event status enable register 3 |  |
:ESE3? |
:ESR0? |  | Reading event status register 0 |  |
:ESR1? |  | Reading event status register 1 |  |
:ESR2? |  | Reading event status register 2 |  |
:ESR3? |  | Reading event status register 3 |  |
## Measurement Mode
:MODE | <LCR/CONTinuous> | Setting and querying measurement mode |  |
:MODE? |
## Measurement Frequency
:FREQuency | <Frequency> | Setting and querying the Measurement Frequency |  |
:FREQuency? |
## Measurement Range
:RANGe | <Range No.> | Setting and querying the measurement range |  |
:RANGe? |
:RANGe:AUTO | <ON/OFF> | Automatically setting and querying the measurement range |  |
:RANGe:AUTO? |
:RANGe:AUTO:LIMit | <RST/lower limit range>,<upper limit range> | Setting and querying the AUTO range limit function |  |
:RANGe:AUTO:LIMit? |
:RANGe:JSYNc | <ON/OFF> | Setting and querying the JUDGE synchronization setting |  |
:RANGe:JSYNc? |
:RANGe:LOWZ | <ON/OFF> | Setting and querying low Z high accuracy mode |  |
:RANGe:LOWZ? |
:RANGe:SYNC | <ON/OFF> | Setting and querying the range synchronization function |  |
:RANGe:SYNC? |
:RANGe:SYNC:AVERaging | <ALL/Range No.>,<OFF/number of averaging times> | Setting and querying the number of measurement averaging time for the range synchronization function |  |
:RANGe:SYNC:AVERaging? | <Range No.>
:RANGe:SYNC:SPEEd | <ALL/Range No.>,<FAST/MEDium/SLOW/SLOW2> | Setting and querying the measurement speed for the range synchronization function |  |
:RANGe:SYNC:SPEEd? | <Range No.>
:RANGe:SYNC:TRIGger:DELay | <ALL/Range No.>,<Trigger delay time> | Setting and querying the trigger delay time for the range synchronization function |  |
:RANGe:SYNC:TRIGger:DELay? | <Range No.>
:RANGe:SYNC:SSOurce | <ALL/Range No.>,<ON/OFF> | Setting and querying the trigger synchronous output function for the range synchronization function |  |
:RANGe:SYNC:SSOurce? | <Range No.>
:RANGe:SYNC:SSOurce:WAIT | <ALL/Range No.>,<Wait time> | Setting and querying the wait time of the trigger synchronous output function for the range synchronization function |  |
:RANGe:SYNC:SSOurce:WAIT? | <Range No.>
## Measurement Signal Level
:LEVel | <V/CV/CC> | Setting and querying the measurement signal level |  |
:LEVel? |
## Constant current level
:LEVel:CCURRent | <Constant current level> | Setting and querying the constant current level value |  |
:LEVel:CCURRent? |
## Constant voltage level
:LEVel:CVOLTage | <Constant voltage level> | Setting and querying the constant voltage level |  |
:LEVel:CVOLTage? |
## Open-circuit voltage level
:LEVel:VOLTage | <Open-circuit voltage level> | Setting and querying the open-circuit voltage level |  |
:LEVel:VOLTage? |
## Measurement Speed
:SPEEd | <FAST/MEDium/SLOW/SLOW2> | Setting and querying the measurement speed |  |
:SPEEd? |
## Limit Function of Measurement Signal Level
:LIMiter | <ON/OFF> | Setting and querying the limit function |  |
:LIMiter? |
:LIMiter:CURRent | <Current limit value> | Setting and querying the current limit value |  |
:LIMiter:CURRent? |
:LIMiter:VOLTage | <Voltage limit value> | Setting and querying the voltage limit value |  |
:LIMiter:VOLTage? |
## Average Function
:AVERaging | <OFF/ number of averaging times> | Setting and querying measurement averaging |  |
:AVERaging? |
## DC bias function
:DCBias | <ON/OFF> | Setting and querying ON/ OFF of DC bias function |  |
:DCBias? |
:DCBias:LEVel | <DC bias level> | Setting and querying the DC bias level |  |
:DCBias:LEVel? |
## Trigger
:TRIGger | <INTernal/EXTernal> | Setting and querying the trigger mode |  |
:TRIGger? |
:TRIGger:DELay | <Trigger delay time> | Setting and querying the trigger delay time |  |
:TRIGger:DELay? |
## Trigger Synchronous Output Function
:SSOurce | <ON/OFF> | Setting and querying the trigger synchronous output function |  |
:SSOurce? |
:SSOurce:WAIT | <Wait time> | Setting and querying the wait time of trigger synchronous output |  |
:SSOurce:WAIT? |
## DC Resistance Measurement Function
:DCResistance:RANGe | <Range No.> | Setting and querying the measurement range for when DC resistance measurement |  |
:DCResistance:RANGe? |
:DCResistance:RANGe:AUTO | <ON/OFF> | Automatically setting and querying the measurement range for when DC resistance measurement |  |
:DCResistance:RANGe:AUTO? |
:DCResistance:RANGe:AUTO:LIMit | <RST/lower limit range>,<upper limit range> | Setting and querying the AUTO range limit function during DC resistance measurement |  |
:DCResistance:RANGe:AUTO:LIMit? |
:DCResistance:RANGe:LOWZ | <ON/OFF> | Setting and querying low Z high accuracy mode for when DC resistance measurement |  |
:DCResistance:RANGe:LOWZ? |
:DCResistance:RANGe:JSYNc | <ON/OFF> | Setting and querying the JUDGE synchronization setting during DC resistance measurement |  |
:DCResistance:RANGe:JSYNc? |
:DCResistance:RANGe:SYNC:AVERaging | <ALL/Range No.>,<OFF/number of averaging times> | Setting and querying the number of measurement averaging time for the range synchronization function during DC resistance measurement |  |
:DCResistance:RANGe:SYNC:AVERaging? | <Range No.>
:DCResistance:RANGe:SYNC:SPEEd | <ALL/Range No.>,<FAST/MEDium/SLOW/SLOW2> | Setting and querying the measurement speed for the range synchronization function during DC resistance measurement |  |
:DCResistance:RANGe:SYNC:SPEEd? | <Range No.>
:DCResistance:SPEEd | <FAST/MEDium/SLOW/SLOW2> | Setting and querying the measurement speed for when DC resistance measurement |  |
:DCResistance:SPEEd? |
:DCResistance:AVERaging | <OFF/ number of averaging times> | Setting and querying averaging for when DC resistance measurement |  |
:DCResistance:AVERaging? |
:DCResistance:ADJust | <ON/OFF> | Setting and querying the DC offset for when DC resistance measurement |  |
:DCResistance:ADJust? |
:DCResistance:ADJust:DEMand |  | Acquiring DC offset for when DC resistance measurement |  |
:DCResistance:ADJDelay | <Adjustment Delay time> | Setting and querying the adjustment delay time during DC resistance measurement |  |
:DCResistance:ADJDelay? |
:DCResistance:DCDelay | <DC Delay time> | Setting and querying the DC delay time during DC resistance measurement |  |
:DCResistance:DCDelay? |
:DCResistance:LFRequency | <Line Frequency> | Setting and querying the line frequency during DC resistance measurement |  |
:DCResistance:LFRequency? |
## Judgment Function
:JUDGment |  | Setting and querying the judgment function |  |
:JUDGment? |
## Comparator Function
:COMParator | <OFF/ON> | Setting and querying ON/ OFF of comparator function |  |
:COMParator? |
:COMParator:FLIMit:ABSolute | <OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the first parameter of the comparator function (absolute value mode) |  |
:COMParator:FLIMit:ABSolute? |
:COMParator:FLIMit:DEViation | <Reference value>,<OFF/ Lower limit values>,<OFF/ Upper limit values> | Setting and querying the reference value and the upper and lower limit values of the first parameter of the comparator function (deviation percentage (ƒ¢%) mode) |  |
:COMParator:FLIMit:DEViation? |
:COMParator:FLIMit:MODE | <ABSolute/PERcent/DEViation> | Setting and querying the judgment mode of the first parameter of the comparator function |  |
:COMParator:FLIMit:MODE? |
:COMParator:FLIMit:PERcent | <Reference value>,<OFF/ Lower limit values>,<OFF/ Upper limit values> | Setting and querying the reference value and the upper and lower limit values of the first parameter of the comparator function (percentage (%) mode) |  |
:COMParator:FLIMit:PERcent? |
:COMParator:SLIMit:ABSolute | <OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the third parameter of the comparator function (absolute value mode) |  |
:COMParator:SLIMit:ABSolute? |
:COMParator:SLIMit:DEViation | <Reference value>,<OFF/ Lower limit values>,<OFF/ Upper limit values> | Setting and querying the reference value and the upper and lower limit values of the SUB parameter of the comparator function (deviation percentage (ƒ¢%) mode) |  |
:COMParator:SLIMit:DEViation? |
:COMParator:SLIMit:MODE | <ABSolute/PERcent/DEViation> | Setting and querying the judgment mode of the third parameter of the comparator function |  |
:COMParator:SLIMit:MODE? |
:COMParator:SLIMit:PERcent | <Reference value>,<OFF/ Lower limit values>,<OFF/ Upper limit values> | Setting and querying the reference value and the upper and lower limit values of the third parameter of the comparator function (percentage mode) |  |
:COMParator:SLIMit:PERcent? |
## BIN Function
:BIN | <OFF/ON> | Setting and querying ON/ OFF of BIN function |  |
:BIN? |
:BIN:FLIMit:ABSolute | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the first parameter of the BIN function (absolute value mode) |  |
:BIN:FLIMit:ABSolute? | <BIN number>
:BIN:FLIMit:DEViation | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the first parameter of the BIN function (deviation percentage (ƒ¢%) mode) |  |
:BIN:FLIMit:DEViation? | <BIN number>
:BIN:FLIMit:MODE | <ABSolute/PERcent/DEViation> | Selecting and querying the mode of the first parameter of the BIN function |  |
:BIN:FLIMit:MODE? |
:BIN:FLIMit:PERcent | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the first parameter of the BIN function (percentage (%) mode) |  |
:BIN:FLIMit:PERcent? | <BIN number>
:BIN:FLIMit:REFerence | <Reference value> | Setting and querying the reference value of the first parameter of the BIN function (percentage (%) mode and deviation percentage (ƒ¢%) mode) |  |
:BIN:FLIMit:REFerence? |
:BIN:SLIMit:ABSolute | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the third parameter of the BIN function (absolute value mode) |  |
:BIN:SLIMit:ABSolute? | <BIN number>
:BIN:SLIMit:DEViation | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the third parameter of the BIN function (deviation percentage (ƒ¢%) mode) |  |
:BIN:SLIMit:DEViation? | <BIN number>
:BIN:SLIMit:MODE | <ABSolute/PERcent/DEViation> | Selecting and querying the mode of the third parameter of the BIN function |  |
:BIN:SLIMit:MODE? |
:BIN:SLIMit:PERcent | <BIN number>,<OFF/ lower value>,<OFF/ upper value> | Setting and querying the upper and lower limit values of the third parameter of the BIN function (percentage (%) mode) |  |
:BIN:SLIMit:PERcent? | <BIN number>
:BIN:SLIMit:REFerence | <Reference value> | Setting and querying the reference value of the third parameter of the BIN function (percentage (%) mode and deviation percentage (ƒ¢%) mode) |  |
:BIN:SLIMit:REFerence? |
## Measurement Value Output
:MEASure? |  | Querying measurement data |  |
:MEASure:OUTPut:AUTO | <ON/OFF> | Setting and querying the measurement value automatic output function |  |
:MEASure:OUTPut:AUTO? |
:MEASure:VALid | <Setting value> | Setting and querying the response data of the measurement acquisition query |  |
:MEASure:VALid? |
:MEASure:ITEM | <MR0>, <MR1>, <MR2> | Setting and querying measurement parameters |  |
:MEASure:ITEM? |
## Parameter Settings (# is a numerical value from 1 to 4)
:PARameter# | <Z/ Y/ PHASE(phase angle)/ CS/ CP/ D/ LS/ LP/ Q/ RS/ G/ RP/ X/ B/ RDC/ S/ E/ OFF> | Setting and querying the display parameters |  |
:PARameter#? |
:PARameter#:DIGit | <Number of display digits> | Setting and querying number of display digits |  |
:PARameter#:DIGit? |
## Open / Short Compensation Range
:CORRection:LIMit:DC | <ON/OFF> | Open / Short compensation function on/off setting and querying during DC measurement |  |
:CORRection:LIMit:DC? |
:CORRection:LIMit:POINt | <UNLimited/Compensation minimum frequency>, <UNLimited/Compensation maximum frequency> | Open / Short compensation range setting and querying during AC measurement |  |
:CORRection:LIMit:POINt? |
## Open-circuit Compensation Function
:CORRection:OPEN | <OFF/ALL/SPOT/CANCel> | Executing, cancelling, and querying the open compensation function |  |
:CORRection:OPEN? |
:CORRection:OPEN:ERRor? |  | Querying open compensation failure flag |  |
:CORRection:OPEN:FREQuency | <Compensation No.>,<OFF/ DC/ Frequency> | Setting and querying frequency for acquiring open compensation value |  |
:CORRection:OPEN:FREQuency? | <Compensation No.>
:CORRection:OPEN:RETurn | <OFF/ALL/SPOT> | Setting and querying the open compensation function |  |
:CORRection:OPEN:RETurn? |
:CORRection:OPEN:DATA:ALL? |  | Open compensation value inquiry (all compensation) |  |
:CORRection:OPEN:DATA:SPOT? | <Compensation No.> | Open compensation value inquiry (spot compensation) |  |
## Short Circuit Compensation Function
:CORRection:SHORt | <OFF/ALL/SPOT/CANCel> | Executing, cancelling, and querying the short compensation function |  |
:CORRection:SHORt? |
:CORRection:SHORt:ERRor? |  | Querying short compensation failure flag |  |
:CORRection:SHORt:FREQuency | <Compensation No.>,<OFF/ DC/ Frequency> | Setting and querying frequency for acquiring short compensation value |  |
:CORRection:SHORt:FREQuency? | <Compensation No.>
:CORRection:SHORt:RETurn | <OFF/ALL/SPOT> | Setting and querying the short compensation function |  |
:CORRection:SHORt:RETurn? |
:CORRection:SHORt:DATA:ALL? |  | Short compensation value inquiry (all compensation) |  |
:CORRection:SHORt:DATA:SPOT? | <Compensation No.> | Short compensation value inquiry (spot compensation) |  |
## Load Compensation Function
:CORRection:LOAD | <OFF/ON> | Executing and querying the load compensation function |  |
:CORRection:LOAD? |
:CORRection:LOAD:CONDition | <Compensation No.>,<Frequency>,<Range No.>,<LOW Z>,<V/ CV /CC>,<Level value>,<DC bias>,<DC bias value> | Setting and querying the load compensation conditions |  |
:CORRection:LOAD:CONDition? | <Compensation No.>
:CORRection:LOAD:DCResistance:CONDition | <Compensation No.>,<Range No.>,<LOW Z> | Setting and querying the load compensation conditions for when DC resistance measurement |  |
:CORRection:LOAD:DCResistance:CONDition? | <Compensation No.>
:CORRection:LOAD:DCResistance:REFerence | <Compensation No.>,<Reference value> | Setting and querying the reference value of load compensation for when DC resistance measurement |  |
:CORRection:LOAD:DCResistance:REFerence? | <Compensation No.>
:CORRection:LOAD:DATA? | <Compensation No.> | Load compensation value inquiry |  |
:CORRection:LOAD:ERRor? |  | Querying load compensation failure flag |  |
:CORRection:LOAD:REFerence | <Compensation No.>,<Mode No.>,<Reference value1>,<Reference value2> | Setting and querying the reference values of load compensation |  |
:CORRection:LOAD:REFerence? | <Compensation No.>
:CORRection:LOAD:RESet | <Compensation No.> | Resetting the load compensation conditions |  |
:CORRection:LOAD:RETurn | <OFF/ON> | Setting and querying the load compensation function |  |
:CORRection:LOAD:RETurn? |
## Cable length compensation function
:CORRection:CABLe | <Cable length> | Setting and querying the cable length compensation function |  |
:CORRection:CABLe? |
## Scaling Function
:CORRection:SCALe | <OFF/ON> | Setting and querying the scaling compensation function |  |
:CORRection:SCALe? |
:CORRection:SCALe:DATA | <Scaling No.>,<Compensation value A>,<Compensation value B> | Setting and querying the scaling compensation value |  |
:CORRection:SCALe:DATA? | <Scaling No.>
## Continuous measurement settings
:CONTinuous:DRAW | <REAL/AFTer> | Setting and querying the screen display timing |  |
:CONTinuous:DRAW? |
:CONTinuous:EXECution | <Panel No.>, <ON/OFF> | Setting and querying the continuous measurement target |  |
:CONTinuous:EXECution? | <Panel No.>
:CONTinuous:COUNt? |  | Panel count targeted for measurement in continuous measurement mode inquiry |  |
## Measurement Value Output
:MEASure? | <No data/ ALL> | Querying measurement data |  |
:MEASure:CONTinuous:COMParator? |  | Querying the overall judgment result when continuous measurement |  |
## Waveform Averaging Function
:WAVE | <ON/OFF> | Setting and querying the waveform averaging function |  |
:WAVE? |
:WAVE:NUM | <Frequency No.>,<number of measurement waveforms> | Setting and querying the number of measurement waveforms for the waveform averaging function |  |
:WAVE:NUM? | <Frequency No.>
:WAVE:RESet | <FAST/MEDium/SLOW/SLOW2> | Resets the number of measurement waveforms for the waveform averaging function to that of each measurement speed. |  |
## Contact Check Function
:CCHeck:VERify | <OFF/BEFore/AFTer/BOTH> | Setting and querying the contact check function |  |
:CCHeck:VERify? |
:CCHeck:SENSitivity | <Settable range> | Setting and querying the settable range for the contact check function |  |
:CCHeck:SENSitivity? |
:CCHeck:DELay | <Delay time> | Setting and querying the contact check delay time |  |
:CCHeck:DELay? |
## HIGH- Z reject function
:HIZ | <ON/OFF> | Setting and querying the Hi Z reject function |  |
:HIZ? |
:HIZ:LIMit | <Limit value> | Setting and querying the limit value of the Hi Z reject function |  |
:HIZ:LIMit? |
## Measurement Value Memory Function
:MEMory? | <No data/ ALL> | Querying measurement values saved to memory with the measurement value memory function |  |
:MEMory:CLEar |  | Clearing memory of measurement value memory function |  |
:MEMory:CONTrol | <ON/IN/OFF> | Setting and querying the measurement value memory function |  |
:MEMory:CONTrol? |
:MEMory:COUNt? |  | Querying the number of measurement values saved to memory with the memory function |  |
:MEMory:POINts | <Memory size> | Setting and querying the measurement value memory size |  |
:MEMory:POINts? |
:MEMory:SAVE |  | Saving of measured value memory |  |
## Display Function
:DISPlay | <ON/OFF> | Setting and querying LCD display |  |
:DISPlay? |
## Zoom Function
:ZOOM | <ON/OFF> | Setting and querying the zoom function |  |
:ZOOM? |
## BCD Output Function
:IO:BCD | <OFF/ON> | Setting and querying ON/ OFF of BCD output function |  |
:IO:BCD? |
:IO:BCD:DECimal | <Parameter No.>, <Decimal point> | Setting and querying decimal point of BCD output function |  |
:IO:BCD:DECimal? | <Parameter No.>
## Key Lock
:KEYLock |  | Executing and querying the key lock |  |
:KEYLock? |
:KEYLock:PASScode | <Passcode/ none> | Setting the key lock passcode |  |
:KEYLock:UNLock | <Passcode/ none> | Disabling the key lock |  |
## Beep Tone
:BEEPer:JUDGment | <OFF/IN/NG> | Setting and querying beep sound for the judgment results of measurement values |  |
:BEEPer:JUDGment? |
:BEEPer:KEY | <ON/OFF> | Setting and querying beep sound for key input |  |
:BEEPer:KEY? |
:BEEPer:TONE | <A/B/C/D> | Setting and querying the beep tone type |  |
:BEEPer:TONE? |
## Calculation Setting of Conductivity/Permittivity
:CALCulate:PARameter | <CS/ CP> | Setting and querying the calculation parameters of conductivity/permittivity |  |
:CALCulate:PARameter? |
:CALCulate:LENGth | <Length of conductor> | Setting and querying the conductor length during calculation of conductivity/permittivity |  |
:CALCulate:LENGth? |
:CALCulate:AREA | <Cross-sectional area of conductor> | Setting and querying the cross-sectional area of the conductor during calculation of conductivity/permittivity |  |
:CALCulate:AREA? |
## Calculation Setting of Conductivity
:SIGMa | <Length of conductor>, <Cross-sectional area of conductor> | Setting and querying the length and cross-sectional area of the conductor during calculation of conductivity |  |
:SIGMa? |
## EXT I/O Output
:IO:EOM:MODE | <HOLD/PULSe> | INDEX and EMO output method setting and inquiry |  |
:IO:EOM:MODE? |
:IO:EOM:PULSe | <Pulse width> | Pulse width for which to keep EOM low (on) setting and inquiry |  |
:IO:EOM:PULSe? |
:IO:OUTPut:DELay | <I/O delay time> | Setting and querying the delay time between judgment result output and EOM output |  |
:IO:OUTPut:DELay? |
:IO:RESult:RESet | <ON/OFF> | Setting and querying output of the judgment result signal line |  |
:IO:RESult:RESet? |
:IO:TRIGger:EDGe | <DOWN/UP> | Setting and querying the trigger edge |  |
:IO:TRIGger:EDGe? |
:IO:TRIGger:ENABle | <ON/OFF> | Setting and querying permit/prohibit of trigger input during measurement |  |
:IO:TRIGger:ENABle? |
## Panel Save Function
:SAVE | <Panel No.>,<Panel name> | Executing and querying the panel save function |  |
:SAVE? | <Panel name>
:SAVE:CLEar | <ALL/ Panel No.> | Clearing data saved for a panel |  |
:SAVE:NAME? | <Panel No.> | Querying a panel name |  |
:SAVE:REName | <Panel No.>,<Panel name> | Changing a panel name |  |
:SAVE:TYPE | <ALL/HARDware/ADJust> | Setting and querying the save type |  |
:SAVE:TYPE? |
:SAVE:MODE? | <Panel No.> | Querying the save type |  |
## Panel Load Function
:LOAD | <Panel No.> | Executing panel load |  |
## Message Terminator
:TRANsmit:TERMinator | <Terminator number> | Setting and querying the terminator of the response message |  |
:TRANsmit:TERMinator? |
## RS-232C Communication Handshake
:HANDshake | <OFF/HARDware/X/BOTH> | Setting and querying the RS-232C Communication Handshake |  |
:HANDshake? |
## Data transfer format
:FORMat:DATA | <ASCii/REAL> | Setting and querying the data transfer format |  |
:FORMat:DATA? |
:FORMat:LONG | <ON/OFF> | Setting and querying long format for when data transfer |  |
:FORMat:LONG? |
## Header
:HEADer | <ON/OFF> | Setting and querying existence of header in response message |  |
:HEADer? |
## System Settings
:SYSTem:DATE | <Year>,<Month>,<Day> | Setting and querying the date |  |
:SYSTem:DATE? |
:SYSTem:MACAddress? |  | Querying the MAC address |  |
:SYSTem:SERIAlno? |  | Querying the serial number |  |
:SYSTem:TIME | <Hour>,<Minute>,<Second> | Setting and querying the time |  |
:SYSTem:TIME? |
:SYSTem:USBId? |  | Returns the USB ID. |  |
## Initialize Device
:PRESet |  | Initializing the instrument |  |
## File storage function
:FILE:DATE | <ON/OFF> | Setting and querying the date and time for when saving text |  |
:FILE:DATE? |
:FILE:DELIMiter | <COMma/TAB/SEMIcolon/SPACE> | Setting and querying the delimiter for when saving text |  |
:FILE:DELIMiter? |
:FILE:FOLDer | <Folder name> | Setting and querying the save folder |  |
:FILE:FOLDer? |
:FILE:INFOrmation? |  | Querying USB flash drive information |  |
:FILE:MODE | <AUTO/MANUAL> | Setting and querying the mode of the save folder |  |
:FILE:MODE? |
:FILE:PANel:SAVE | <Panel name> | Execution of panel save to USB memory |  |
:FILE:PANel:LOAD | <Panel name> | Execution of panel load from USB memory |  |
:FILE:PANel:ALLSave | <Specified save folder name> | Execution of all save to USB memory |  |
:FILE:PANel:ALLLoad | <Specified save folder name> | Execution of all load from USB memory |  |
:FILE:PARAmeter | <ON/OFF> | Setting and querying the measurement parameter setting for when saving text |  |
:FILE:PARAmeter? |
:FILE:QUOTe | <OFF/DOUBle/SINGle> | Setting and querying the quotation mark setting for when saving text |  |
:FILE:QUOTe? |
:FILE:SAVE |  | Executing file saving |  |
:FILE:SET | <ON/OFF> | Setting and querying the measurement condition setting for when saving text |  |
:FILE:SET? |
:FILE:TYPE:TEXT | <OFF/ON> | Text save settings and inquiry |  |
:FILE:TYPE:TEXT? |
:FILE:TYPE:BMP | <OFF/COLor/MONochrome> | BMP save settings and inquiry |  |
:FILE:TYPE:BMP? |
## Monitor Function
:MONItor? |  | Querying the voltage/current monitor value |  |
## Screen storage function
:HCOPy:DATA? | <COLor/MONochrome> | Acquiring the BMP data of the measurement screen |  |