Configuration (CONFigure)

Sets and queries the title comment addition for auto save file name.
Syntax | (Command) (Query) | :CONFigure:ADDComment A$ :CONFigure:ADDComment?
(Response) | A$ A$ = OFF, ON
Details | Sets the title comment addition for auto save file name. Returns the current setting of the title comment addition for auto save file name.
OFF | Do not add title comment（Automatically add numbers）
ON | Add title comment
Example | :CONFigure:ADDComment ON :CONFigure:ADDComment? (Response) :CONFIGURE:ADDComment ON (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the trigger date addition for auto save file name.
Syntax | (Command) (Query) | :CONFigure:ADDDate A$ :CONFigure:ADDDate?
(Response) | A$ A$ = OFF, ON
Details | Sets the trigger date addition for auto save file name. Returns the current setting of the trigger date addition for auto save file name.
OFF | Do not add trigger date（Automatically add numbers）
ON | Add trigger date
Example | :CONFigure:ADDDate ON :CONFigure:ADDDate? (Response) :CONFIGURE:ADDDATE ON (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the alarm source saving.
Syntax | (Command) (Query) | :CONFigure:ALMSource A$ :CONFigure:ALMSource?
(Response) | A$ A$ = OFF, ON
Details | Sets the alarm source saving. Returns the current setting of the alarm source saving.
OFF | Do not save alarm source data.
ON | Save alarm source data.
Example | :CONFigure:ALMSource ON :CONFigure:ALMSource? (Response) :CONFIGURE:ALMSOURCE ON (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the auto save function.
Syntax | (Command) (Query) | :CONFigure:ATSAve A$(,"B$") :CONFigure:ATSAve?
(Response) | A$(,"B$") A$ = OFF, BIN, CSV, MF4, MEAS, BIN_MEAS, CSV_MEAS, MF4_MEAS B$ = file name (up to 8 characters)(can be omitted)
Details | Sets the auto save function. Omit B$ only when A$ = OFF. Returns the auto save function as character data.
OFF | Waveform Data：No Save | Numerical Calculation Data：No Save
BIN | Waveform Data：Save binary format | Numerical Calculation Data：No Save
CSV | Waveform Data：Save text format | Numerical Calculation Data：No Save
MF4 | Waveform Data：Save MF4 format | Numerical Calculation Data：No Save
MEAS | Waveform Data：No Save | Numerical Calculation Data：Save text format
BIN_MEAS | Waveform Data：Save binary format | Numerical Calculation Data：Save text format
CSV_MEAS | Waveform Data：Save text format | Numerical Calculation Data：Save text format
MF4_MEAS | Waveform Data：Save MF4 format | Numerical Calculation Data：Save text format
Example | :CONFigure:ATSAve BIN,"AUTO" :CONFigure:ATSAve? (Response) :CONFIGURE:ATSAVE BIN,"AUTO" (when headers are enabled)
Note | Waveform data save format can be set by :SAVEWave command. Numerical calculation data save format can be set by :SAVECalc command. File name can be set by :FILEName command. The characters that can be used in the file name are the same as those of the main unit.
Usage Conditions | -

Sets and queries the folder Splitting for auto save.
Syntax | (Command) (Query) | :CONFigure:AUTOFolder A$ :CONFigure:AUTOFolder?
(Response) | A$ A$ = OFF, DAY, WEEK, MONTH
Details | Sets folder Splitting for auto save. Returns the current setting of the folder Splitting for auto save.
OFF | No Splitting
DAY | 1 Day
WEEK | 1 Week
MONTH | 1 Month
Example | :CONFigure:AUTOFolder DAY :CONFigure:AUTOFolder? (Response) :CONFIGURE:AUTOFOLDER DAY (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the file name for auto save.
Syntax | (Command) (Query) | :CONFigure:FILEName "A$" :CONFigure:FILEName?
(Response) | "A$" A$ = file name (up to 8 characters)
Details | Sets file name for auto save. Returns a string of file name for auto save.
Example | :CONFigure:FILEName "ABC" :CONFigure:FILEName? (Response) :CONFIGURE:FILENAME "ABC" (when headers are enabled)
Note | File name can be set by :ATSAve command. Characters exceeding the maximum number of characters are not set. The characters that can be used in the file name are the same as those of the main unit.
Usage Conditions | The auto save function setting must be set to something other than OFF.

Execute the Setting conditions file load and queries the result.
Syntax | (Query) | :CONFigure:LOAD? A,B
(Response) | C<NR1> A = 1 to 5 B = 0 to 3(Load option number) C = 0(PASS),1(FAIL)
Details | Execute the Setting conditions file load on the ROM and queries the result. The type of settings to load setting on the specified load option number. Load option
B=0 | Wired unit information
B=1 | Wired unit information + System,External
B=2 | Wired unit information + Wireless unit information
B=3 | Wired unit information + System,External + Wireless unit information
Example | :CONFigure:LOAD? 1,1 (Response) :CONFIGURE:LOAD 0 (when headers are enabled)
Note | The configuration condition file cannot be imported during measurement.
Usage Conditions | -

Sets and queries the number display format.
Syntax | (Command) (Query) | :CONFigure:NUMFormat A$ :CONFigure:NUMFormat?
(Response) | A$ A$ = STANDARD, DECIMAL, EXPONENT, PREFIX
Details | Sets the number display format. Returns the current setting of the number display format.
STANDARD | Standard
DECIMAL | Decimal
EXPONENT | Exponent
PREFIX | Prefix
Example | :CONFigure:NUMFormat STANDARD :CONFigure:NUMFormat? (Response) :CONFIGURE:NUMFORMAT STANDARD (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the recording time.
Syntax | (Command) (Query) | :CONFigure:RECTime day,hour,min,sec :CONFigure:RECTime?
(Response) | day<NR1>,hour<NR1>,min<NR1>,sec<NR1> day = 0 to 500 (day) hour = 0 to 23 (hour) min = 0 to 59 (min) sec = 0 to 59 (sec)
Details | Sets the recording time to a numerical value. Returns the currently set value of the recording time as an NR1 numerical value. If all parameters are 0, the recording time is continuous.
Example | :CONFigure:RECTime 0,0,0,10 :CONFigure:RECTime? (Response) :CONFIGURE:RECTIME 0,0,0,10 (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the recording interval.
Syntax | (Command) (Query) | :CONFigure:SAMPle A :CONFigure:SAMPle?
(Response) | A<NR3> (1 decimal places) A = 1.0E-3 to 3.6E+3 (sec)
Details | Sets the recording interval to a numerical value (unit seconds). Returns the currently set value of the recording interval as an NR3 numerical value.
Example | :CONFigure:SAMPle 1E-2 :CONFigure:SAMPle? (Response) :CONFIGURE:SAMPLE 1.0E-02 (when headers are enabled)
Note | If an attempt is made to set the horizontal axis to a non-permitted value, and there is a range above that value, that range will be selected.
Usage Conditions | -

Sets and queries the format for saving mathematical results.
Syntax | (Command) (Query) | :CONFigure:SAVECalc A$ :CONFigure:SAVECalc?
(Response) | A$ A$ = OFF, CSV
Details | Sets the format for saving mathematical results by the auto save function. Returns the current setting of the format for saving mathematical results.
OFF | No Save
CSV | Save text format
Example | :CONFigure:SAVECalc CSV :CONFigure:SAVECalc? (Response) :CONFIGURE:SAVECALC CSV (when headers are enabled)
Note | Numerical calculation data save format can be set by :ATSAve command.
Usage Conditions | -

Sets and queries the text save decimal.
Syntax | (Command) (Query) | :CONFigure:SAVEDeci A$ :CONFigure:SAVEDeci?
(Response) | A$ A$ = PERIOD, COMMA
Details | Sets the text save decimal when data is stored in text format by the auto save function. Returns the current setting of the text save decimal as character data.
PERIOD | Use Period
COMMA | Use Comma
Example | :CONFigure:SAVEDeci PERIOD :CONFigure:SAVEDeci? (Response) :CONFIGURE:SAVEDECI PERIOD (when headers are enabled)
Note | When save separator is COMMA, save decimal cannot be set to COMMA.
Usage Conditions | -

Sets and queries the text save date format.
Syntax | (Command) (Query) | :CONFigure:SAVEFormat A$ :CONFigure:SAVEFormat?
(Response) | A$ A$ = COMMENT, SPLITMS, LOCALCOMMENT, LOCALSPLITMS
Details | Sets the text save date format when data is stored in text format by the auto save function. Returns the current setting of the text save date format as character data.
COMMENT | yy-MM-dd hh:mm:ss.0
SPLITMS | yyyy-MM-dd hh:mm:ss + ms
LOCALCOMMENT | Localized COMMENT
LOCALSPLITMS | Localized SPLITMS
Example | :CONFigure:SAVEFormat COMMENT :CONFigure:SAVEFormat? (Response) :CONFIGURE:SAVEFORMAT COMMENT (when headers are enabled)
Note | LOCALCOMMENT, LOCALSPLITMS can only be specified if MMDDYYYY, DDMMYYYY is specified in :SYSTem:DFORmat or SLASH, PERIOD is specified in :SYSTem:DSEParator.
Usage Conditions | -

Sets and queries the auto save division.
Syntax | (Command) (Query) | :CONFigure:SAVEKind A$ :CONFigure:SAVEKind?
(Response) | A$ A$ = NORMal, DIVide,REGUlarly
Details | Sets the auto save division when data is stored by the auto save function. Returns the current setting of the realtime save division as character data.
NORMal | Disable
DIVide | Enable
REGUlarly | Fix Time
Example | :CONFigure:SAVEKind NORMal :CONFigure:SAVEKind? (Response) :CONFIGURE:SAVEKIND NORMAL (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the realtime save division length.
Syntax | (Command) (Query) | :CONFigure:SAVELen day,hour,min :CONFigure:SAVELen?
(Response) | day<NR1>,hour<NR1>,min<NR1> day = 0 to 30 (day) hour = 0 to 23 (hour) min = 0 to 59 (min)
Details | Sets the auto save division length to a numerical value. Returns the currently set value of the realtime save division length as an NR1 numerical value.
Example | :CONFigure:SAVELen 0,0,10 :CONFigure:SAVELen? (Response) :CONFIGURE:SAVELEN 0,0,10 (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the realtime save mode.
Syntax | (Command) (Query) | :CONFigure:SAVEMode A$ :CONFigure:SAVEMode?
(Response) | A$ A$ = FILEfull, REMove
Details | Sets the realtime save mode when data is stored by the auto save function. Returns the current setting of the auto save mode as character data.
FILEfull | OFF：If a media becomes full auto save is ended.
REMove | ON ：If a media becomes full remove oldest data file before saving.
Example | :CONFigure:SAVEMode FILEfull :CONFigure:SAVEMode? (Response) :CONFIGURE:SAVEMODE FILEFULL (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the realtime save priority.
Syntax | (Command) (Query) | :CONFigure:SAVEPri A$ :CONFigure:SAVEPri?
(Response) | A$ A$ = SD, USB
Details | Sets the realtime save priority when data is stored by the auto save function. Returns the current setting of the realtime save priority as character data.
SD | SD Memory Card
USB | USB flash drive
Example | :CONFigure:SAVEPri SD :CONFigure:SAVEPri? (Response) :CONFIGURE:SAVEPRI SD (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the reference time for autosave file splitting
Syntax | (Command) (Query) | :CONFigure:SAVEReg hour,min :CONFigure:SAVEReg?
(Response) | hour<NR1>,min<NR1> hour = 0 to 23 (hour) min = 0 to 59 (min)
Details | Set the reference time of the autosave file splitting function. Returns the setting for the current autosave file split as a NR1 number.
Example | :CONFigure:SAVEReg 0,0 :CONFigure:SAVEReg? (Response) :CONFIGURE:SAVEREG 0,0 (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the text save separator.
Syntax | (Command) (Query) | :CONFigure:SAVESep A$ :CONFigure:SAVESep?
(Response) | A$ A$ = COMMA, SPACE, TAB, SEMI
Details | Sets the text save separator when data is stored in text format by the auto save function. Returns the current setting of the text save separator as character data.
COMMA | Use Comma
SPACE | Use Space
TAB | Use Tab
SEMI | Use Semicolon
Example | :CONFigure:SAVESep COMMA :CONFigure:SAVESep? (Response) :CONFIGURE:SAVESEP COMMA (when headers are enabled)
Note | When save decimal is COMMA, save separator cannot be set to COMMA.
Usage Conditions | -

Sets and queries the split time for autosave file splits
Syntax | (Command) (Query) | :CONFigure:SAVETime A :CONFigure:SAVETime?
(Response) | A<NR1> A = 1,2,5,10,15,20,30,60(1hour),120(2hour),180(3hour),240(4hour),360(6hour),480(8hour),720(12hour),1440(1day) (unit min)
Details | Sets the split time for autosave file splits as a numeric value. Returns the current split time of the autosave file split as an NR1 number.
Example | :CONFigure:SAVETime 1 :CONFigure:SAVETime? (Response) :CONFIGURE:SAVETIME 1 (when headers are enabled)
Note | If you specify a value that is not in the setting, it will be set to the nearest split time if there is a longer split time than the value you tried to set.
Usage Conditions | -

Sets and queries the format for saving waveform Data.
Syntax | (Command) (Query) | :CONFigure:SAVEWave A$ :CONFigure:SAVEWave?
(Response) | A$ A$ = OFF, BIN, CSV, MF4
Details | Sets the format for saving waveform data by the auto save function. Returns the current setting of the format for saving waveform data.
OFF | No Save
BIN | Save binary format
CSV | Save text format
MF4 | MF4 format
Example | :CONFigure:SAVEWave BIN :CONFigure:SAVEWave? (Response) :CONFIGURE:SAVEWAVE BIN (when headers are enabled)
Note | Waveform data save format can be set by :ATSAve command.
Usage Conditions | -

Sets and queries the measurement start.
Syntax | (Command) (Query) | :CONFigure:STARt A$ :CONFigure:STARt?
(Response) | A$ A$ = MANUAL, TIME
Details | Sets the measurement start. Returns the current setting of measurement start.
MANUAL | Unreserved
TIME | Reservation time
Example | :CONFigure:STARt MANUAL :CONFigure:STARt? (Response) :CONFIGURE:START MANUAL (when headers are enabled)
Note | The measurement start cannot be setted during measurement.
Usage Conditions | -

Sets and queries the measurement start time.
Syntax | (Command) (Query) | :CONFigure:STARTTime year,month,day,hour,minute :CONFigure:STARTTime?
(Response) | year<NR1>,month<NR1>,day<NR1>hour<NR1>,minute<NR1> year = 21～37 (year) month = 1～12 (month) day = 1～31 (day) hour = 0～23（hour） minute = 0～59（minute）
Details | Sets the measurement start. Returns the current setting of measurement start time.
Example | :CONFigure:STARTTime 21,1,2,12,34 :CONFigure:STARTTime? (Response) :CONFIGURE:STARTTIME 21,1,2,12,34 (when headers are enabled)
Note | The measurement start time cannot be setted during measurement. The measurement start time cannot be set to a time later than the measurement stop time.
Usage Conditions | -

Sets and queries the measurement stop.
Syntax | (Command) (Query) | :CONFigure:STOP A$ :CONFigure:STOP?
(Response) | A$ A$ = MANUAL, TIME
Details | Sets the measurement stop. Returns the current setting of measurement stop.
MANUAL | Unreserved
TIME | Reservation time
Example | :CONFigure:STOP MANUAL :CONFigure:STOP? (Response) :CONFIGURE:STOP MANUAL (when headers are enabled)
Note | The measurement stop cannot be setted during measurement.
Usage Conditions | -

Sets and queries the measurement stop time.
Syntax | (Command) (Query) | :CONFigure:STOPTime year,month,day,hour,minute :CONFigure:STOPTime?
(Response) | year<NR1>,month<NR1>,day<NR1>hour<NR1>,minute<NR1> year = 21～37 (year) month = 1～12 (month) day = 1～31 (day) hour = 0～23（hour） minute = 0～59（minute）
Details | Sets the measurement stop. Returns the current setting of measurement stop time.
Example | :CONFigure:STOPTime 21,1,2,12,34 :CONFigure:STOPTime? (Response) :CONFIGURE:STOPTIME 21,1,2,12,34 (when headers are enabled)
Note | The measurement stop time cannot be setted during measurement. The measurement stop time cannot be set to a time earlier than the measurement start time.
Usage Conditions | -

Sets and queries the synchronous operation.
Syntax | (Command) (Query) | :CONFigure:SYNCSet A$ :CONFigure:SYNCSet?
(Response) | A$ A$ = OFF, PRIMary, SECondary
Details | Sets the Primary, Secondary, and off for synchronous operation. Returns the current setting of the synchronous operation.
OFF | Do not perform synchronous operation
PRIMary | Primary
SECondary | Secondary
Example | :CONFigure:SYNCSet PRIMary :CONFigure:SYNCSet? (Response) :CONFIGURE:SYNCSET PRIMARY (when headers are enabled)
Note | Synchronous operation cannot be set during monitoring or measurement.
Usage Conditions | -

Sets and queries the horizontal axis.
Syntax | (Command) (Query) | :CONFigure:TDIV A :CONFigure:TDIV?
(Response) | A<NR3> (2 decimal places) A = 2.00E-03 to 8.64E+04 (sec)
Details | Sets the horizontal axis to a numerical value (unit seconds). Returns the currently set value of the horizontal axis as an NR3 numerical value.
Example | :CONFigure:TDIV 1E-01 :CONFigure:TDIV? (Response) :CONFIGURE:TDIV 1.00E-01 (when headers are enabled)
Note | If an attempt is made to set the horizontal axis to a non-permitted value, and there is a range above that value, that range will be selected.
Usage Conditions | -

Sets and queries the downsampling type for auto save
Syntax | (Command) (Query) | :CONFigure:THINData A$ :CONFigure:THINData?
(Response) | A$ A$ = INSTANT, STATISTICS
Details | Sets the downsampling type for auto save Returns the downsampling type for auto save
INSTANT | Instant value
STATISTICS | Statistics value
Example | :CONFigure:THINData INSTANT :CONFigure:THINData? (Response) :CONFIGURE:THINDATA INSTANT (when headers are enabled)
Note | -
Usage Conditions |

Sets and queries the decimation factor for auto save.
Syntax | (Command) (Query) | :CONFigure:THINOut A :CONFigure:THINOut?
(Response) | A<NR1> A = 1(OFF) to 100000
Details | Sets the decimation factor for auto save. Returns the currently set value of the decimation factor as an NR1 numerical value. If A=1, downsampling is off.
Example | :CONFigure:THINOut 1000 :CONFigure:THINOut? (Response) :CONFIGURE:THINOUT 1000 (when headers are enabled)
Note | -
Usage Conditions | -