Cursor (CURSor)

Command | Data (for a query, response data) | Explanation
:ABCUrsor A$ | A$ = A, B, A_B | Selects among the A, B and A&B cursors Queries
:ABCUrsor? | A$
:APOSition A | A = Cursor Position | Sets the position of the A cursor Queries
:APOSition? | A<NR1>
:BPOSition A | A = Cursor Position | Sets the position of the B cursor Queries
:BPOSition? | A<NR1>
:DISP A$ | A$ = A_B, A_BA, B_BA,A_COMM, B_COMM, BA_COMM | Sets the display of AB cursor values Queries
:DISP? | A$
:MODE A$ | A$ = TIME, VOLT | Sets the A and B cursor type Queries
:MODE? | A$
:READ? ch$,A$ | B$ ch$ = , , , , A$ = A, B, B_A, C, D, D_C B$ = readout value(V) | Queries the cursor readout value for each channel
X-Y Synthesis(:CURSor:XY)
:CDCUrsor A$,B$ | A$ = TRACE, CROSS B$ = C, D, C_D | Selects among the C, D and C&D cursors Queries
:CDCUrsor? A$ | A$,B$
:CH A$,xy$ | A$ = CCURSOR, DCURSOR xy$ = | Sets the target channel of the trace cursor Queries
:CH? A$ | A$,xy$
:CPOSition A | A = Cursor Position | Sets the position of the C cursor Queries
:CPOSition? | A<NR1>
:DISP A$ | A$ = C_D, C_DC, D_DC,C_COMM, D_COMM, DC_COMM | Sets the display of C and D cursor values Queries
:DISP? | A$
:DPOSition A | A = Cursor Position | Sets the position of the D cursor Queries
:DPOSition? | A<NR1>
:KIND A$ | A$ = OFF, TRACE, CROSS | Sets the C and D cursor type Queries
:KIND? | A$
:MODE A$ | A$ = X, Y | Sets the C and D cursor axis Queries
:MODE? | A$
:SELect A$ | A$ = ALL_CH, CH_SET | Sets the cursor channel mode Queries
:SELect? | A$