Calculations (CALCulate)

Command | Data (for a query, response data) | Explanation
Numerical Calculation (:CALCulate:MEAS)
:MEASure A$ | A$ = OFF, ON, EXEC | Sets numerical calculation Queries
:MEASure? | A$
:ANSWer? no$,ch$ | no$,ch$,A<NR3> (5 decimal places) no$ = NO1 to NO10 ch$ = , , A = Calculation Result | Queries result of a numerical calculation
:AREA A$ | A$ = ALL, AB, TOP_A, TOP_B, A_END, B_END | Sets calculation area Queries
:AREA? | A$
:DISP A$ | A$ = USUAL, SPLIT | Sets calculation result display kind Queries
:DISP? | A$
:FILE A$ | A$ = OFF, ON | Sets calculation file divisionses Queries
:FILE? | A$
:INTegra no$,A$ | no$ = NO1 to NO10 A$ = TOTAL,POSitive,NEGative,ABSolute | Sets accumulation/integrations method Queries
:INTegra? no$ | no$,A$
:KIND A$ | A$ = OFF, DIVide, ONTIME | Sets time split calculation kind Queries
:KIND? | A$
:LEN day,hour,min | day = 0 to 30(day) hour = 0 to 23(hour) min = 0 to 59(min) | Sets time split calculation division length Queries
:LEN? | day<NR1>,hour<NR1>,min<NR1>
:LEVEl ch$,A | ch$ = , , A = -9.9999E+29~+9.9999E+29 | Sets thresholds for Numerical Calculation Queries
:LEVEl? ch$ | ch$,A<NR3> (4 decimal places)
:REG hour,min | hour = 0 to 23(hour) min = 0 to 59(min) | Sets time split calculation regular time Queries
:REG? | hour<NR1>,min<NR1>
:SET no$,A$ | no$ = NO1 to NO10 A$ = OFF, AVE, PP, MAX, MIN, MAXT, MINT, ACC, INT, OPE, ONT, OFFT, ONC, OFFC | Sets numerical calculation item Queries
:SET? no$ | no$,A$
:TARGet no$,ch$ | no$ = NO1 to NO10 ch$ = ALL, , , | Sets calculation target channel Queries
:TARGet? no$ | no$,ch$
:TIME A | A = 1, 2, 5, 10, 15, 20, 30, 60, 120, 180, 240, 360, 480, 720, 1440 (unit min) | Sets time split calculation division time
:TIME? | A<NR1> (unit min)
Waveform Calculation (:CALCulate:WAVE)
:KIND w$,A$ | w$ = A$ = OPE, SUM, AVE, MOV, INT | Sets wave calculation kind Queries
:KIND? w$ | w$,A$
:STR w$,"A$" | w$ = A$ = wave calc unit(7 character) | Sets wave calculation unit Queries
:STR? w$ | w$,"A$"
Four arithmetic (:CALCulate:WAVE:ARIThmetic)
Four arithmetic：Coefficients (:CALCulate:WAVE:ARIThmetic:COEF)
:A w$,A | w$ = A = -9.9999E+29 to 9.9999E+29 | Sets four arithmetic coefficient A Queries
:A? w$ | w$,A<NR3> (4 decimal places)
:B w$,A | w$ = A = -9.9999E+29 to 9.9999E+29 | Sets four arithmetic coefficient B Queries
:B? w$ | w$,A<NR3> (4 decimal places)
:C w$,A | w$ = A = -9.9999E+29 to 9.9999E+29 | Sets four arithmetic coefficient C Queries
:C? w$ | w$,A<NR3> (4 decimal places)
:D w$,A | w$ = A = -9.9999E+29 to 9.9999E+29 | Sets four arithmetic coefficient D Queries
:D? w$ | w$,A<NR3> (4 decimal places)
:E w$,A | w$ = A = -9.9999E+29 to 9.9999E+29 | Sets four arithmetic coefficient E Queries
:E? w$ | w$,A<NR3> (4 decimal places)
Four arithmetic：Operator (:CALCulate:WAVE:ARIThmetic:OPERator)
:A w$,A$ | w$ = A$ = OFF, PLUS, MINUS, MULTI, DIV | Sets four arithmetic operator A Queries
:A? w$ | w$,A$
:B w$,A$ | w$ = A$ = OFF, PLUS, MINUS, MULTI, DIV | Sets four arithmetic operator B Queries
:B? w$ | w$,A$
:C w$,A$ | w$ = A$ = OFF, PLUS, MINUS, MULTI, DIV | Sets four arithmetic operator C Queries
:C? w$ | w$,A$
:D w$,A$ | w$ = A$ = OFF, PLUS, MINUS, MULTI, DIV, EXP | Sets four arithmetic operator D Queries
:D? w$ | w$,A$
Moving Average (:CALCulate:WAVE:MOVe)
:POINt w$,A | w$ = A = 1 to 600 (point) | Sets moving average point Queries
:POINt? w$ | w$,A<NR1>
Reset Setting for Integral and Simple Average (:CALCulate:WAVE:RESet)
:BASE w$,hour,min | w$ = hour = 0 to 23 (hour) min = 0 to 59 (min) | Set reset referense time Queries
:BASE? w$ | w$,hour<NR1>,min<NR1>
:INT w$,day,hour,min | w$ = day = 0 to 30 (day) hour = 0 to 23 (hour) min = 0 to 59 (min) | Sets reset interval Queries
:INT? w$ | w$,day<NR1>,hour<NR1>,min<NR1>
:KIND w$,A$ | w$ = A$ = OFF, TRIG | Sets reset timing Queries
:KIND? w$ | w$,A$
:TIME w$,A$ | w$ = A$ = OFF, ON, ONTIME | Sets reset time Queries
:TIME? w$ | w$,A$
Source Channel (:CALCulate:WAVE:SOURce)
:SR1 w$,ch$ | w$ = ch$ =, , | Sets wave calculation source A Queries
:SR1? w$ | w$,ch$
:SR2 w$,ch$ | w$ = ch$ =, , | Sets wave calculation source B Queries
:SR2? w$ | w$,ch$
:SR3 w$,ch$ | w$ = ch$ =, , | Sets wave calculation source C Queries
:SR3? w$ | w$,ch$
:SR4 w$,ch$ | w$ = ch$ =, , | Sets wave calculation source D Queries
:SR4? w$ | w$,ch$
XY Synthesis (:CALCulate:XY)
:AREA A$ | A$ = ALL, AB | Sets XY Synthesis area. Queries
:AREA? | A$
:INTerpolation A$ | A$ = DOT, LINE | Sets XY Synthesis interpolation. Queries
:INTerpolation? | A$
:SYNThesis A$ | A$ = OFF, ON, REDRAW | Sets XY Synthesis. Queries
:SYNThesis? | A$