Alarm (ALARm)

Command | Data (for a query, response data) | Explanation
:ACTive alm$,A$ | alm$ = A$ = LOW, HIGH | Sets alarm output terminal Queries
:ACTive? alm$ | alm$,A$
:ARCD? NO | NO,ALM$,CH$,ERR$,STR$,END$ NO = alarm history num ALM$ = , COM CH$ = , ERR$ = -, BURN_OUT, BATT_LOW, BURN/BATT, DISCONNECT STR$ = alarm start time END$ = alarm stop time | Queries the alarm history details
:ARCDNum? | A<NR1> = 0 to 999999 (0 = none) | Queries the alarm history num
:BATT alm$,A$ | alm$ = A$ = OFF, ON | Sets alarm at low battery Queries
:BATT? alm$ | alm$,A$
:BEEP A$ | A$ = OFF, ON | Sets alarm beep sound Queries
:BEEP? | A$
:BURN alm$,A$ | alm$ = A$ = OFF, ON | Sets alarm at burn out Queries
:BURN? alm$ | alm$,A$
:DISCon alm$,A$ | alm$ = A$ = OFF, ON, DELAY | Sets alarm at communication disconnect Queries
:DISCon? alm$ | alm$,A$
:FILTer alm$,A | alm$ = A = 0(OFF), 2 to 1000 | Sets alarm filter Queries
:FILTer? alm$ | alm$,A<NR1>
:HISTory A$ | A$ = OFF, ON | Sets the alarm history recording Queries
:HISTory? | A$
:HOLD A$ | A$ = OFF, ON, CLEAR | Sets alarm hold Queries
:HOLD? | A$
:SOURce alm$,A$ | alm$ = A$ = AND, OR | Sets alarm source AND/OR Queries
:SOURce? alm$ | alm$,A$
Analog Channel Alarm (:ALARm:ANALog)
:KIND alm$,ch$,A$ | alm$ = ch$ = A$ = OFF, LEVEl, WINDow, SLOPe, SLOPE2 | Sets type of alarm Queries
:KIND? alm$,ch$ | alm$,ch$,A$
:LEVEl alm$,ch$,A | alm$ = ch$ = A = alarm level | Sets the alarm level of the level alarm Queries
:LEVEl? ch$ | alm$,ch$,A<NR3> (3 decimal places)
:LOWEr alm$,ch$,A | alm$ = ch$ = A = lower limit level | Sets lower limit level of window-in/-out alarm Queries
:LOWEr? alm$,ch$ | alm$,ch$,A<NR3> (3 decimal places)
:SIDE alm$,ch$,A$ | alm$ = ch$ = A$ = IN, OUT | Sets the alarm side(window alarm) Queries
:SIDE? alm$,ch$ | alm$,ch$,A$
:SLOPe alm$,ch$,A$ | alm$ = ch$ = A$ = HIGH, LOW | Sets the alarm slope(level alarm) Queries
:SLOPe? alm$,ch$ | alm$,ch$,A$
:SLP2:TIMe alm$,ch$,hour,min,sec,ms | alm$ = ch$ = hour = 0～23(hour) min = 0～59(min) sec = 0～59(sec) ms = 0～999(millisec) | Sets the time of alarm change amount Queries
:SLP2:TIMe? alm$,ch$ | alm$,ch$,hour<NR1>,min<NR1>,sec<NR1>,ms<NR1>
:STIMe alm$,ch$,hour,min,sec | alm$ = ch$ = hour = 0 to 6(hour) min = 0 to 59(min) sec = 0 to 59(sec) | Sets time width of slope alarm Queries
:STIMe? alm$,ch$ | alm$,ch$,hour<NR1>,min<NR1>,sec<NR1>
:UPPEr alm$,ch$,A | alm$ = ch$ = A = upper limit level | Sets upper limit level of window-in/-out alarm Queries
:UPPEr? alm$,ch$ | alm$,ch$,A<NR3> (3 decimal places)
Waveform Calculation Alarm (:ALARm:CALCulate)
:KIND alm$,w$,A$ | alm$ = w$ = A$ = OFF, LEVEl, WINDow, SLOPe, SLOPE2 | Sets type of alarm Queries
:KIND? alm$,w$ | alm$,w$,A$
:LEVEl alm$,w$,A | alm$ = w$ = A = alarm level(-9.9999E+29 to 9.9999E+29) | Sets the alarm level of the level alarm Queries
:LEVEl? alm$,w$ | alm$,w$,A<NR3> (4 decimal places)
:LOWEr alm$,w$,A | alm$ = w$ = A = lower limit level(-9.9999E+29 to 9.9999E+29) | Sets lower limit level of window-in/-out alarm Queries
:LOWEr? alm$,w$ | alm$,w$,A<NR3> (4 decimal places)
:SIDE alm$,w$,A$ | alm$ = w$ = A$ = IN, OUT | Sets the alarm side(window alarm) Queries
:SIDE? alm$,w$ | alm$,w$,A$
:SLOPe alm$,w$,A$ | alm$ = w$ = A$ = HIGH, LOW | Sets the alarm slope(level alarm) Queries
:SLOPe? alm$,w$ | alm$,w$,A$
:SLP2:TIMe alm$,w$,hour,min,sec,ms | alm$ = w$ = hour = 0～23(hour) min = 0～59(minute) sec = 0～59(sec) ms = 0～999(millisec) | Sets he time of alarm change amount Queries
:SLP2:TIMe? alm$,w$ | alm$,w$,hour<NR1>,min<NR1>,sec<NR1>,ms<NR1>
:STIMe alm$,w$,hour,min,sec | alm$ = w$ = hour = 0 to 6(hour) min = 0 to 59(min) sec = 0 to 59(sec) | Sets time width of slope alarm Queries
:STIMe? alm$,w$ | alm$,w$,hour<NR1>,min<NR1>,sec<NR1>
:UPPEr alm,w$,A | alm$ = w$ = A = upper limit level(-9.9999E+29 to 9.9999E+29) | Sets upper limit level of window-in/-out alarm
:UPPEr? alm$,w$ | alm$,w$,A<NR3> (4 decimal places)
CAN Channel Alarm (:ALARm:CAN)
:KIND no$,alm$,A$ | no$ = alm$ = A$ = OFF, LEVEl, WINDow, SLOPe, SLOPE2 | Sets type of alarm Queries
:KIND? no$,alm$ | no$,alm$,A$
:LEVEl no$,alm$,A | no$ = alm$ = A = alarm level | Sets the alarm level of the level alarm Queries
:LEVEl? ch$ | no$,alm$,A<NR3> (3 decimal places)
:LOWEr no$,alm$,A | no$ = alm$ = A = lower limit level | Sets lower limit level of window-in/-out alarm Queries
:LOWEr? no$,alm$ | no$,alm$,A<NR3> (3 decimal places)
:NO no$,ch$ | no$ = ch$ = OFF, | Sets the CAN channels of the alarm number Queries
:NO? no$ | no$,ch$
:SIDE no$,alm$,A$ | no$ = alm$ = A$ = IN, OUT | Sets the alarm side(window alarm) Queries
:SIDE? no$,alm$ | no$,alm$,A$
:SLOPe no$,alm$,A$ | no$ = alm$ = A$ = HIGH, LOW | Sets the alarm slope(level alarm) Queries
:SLOPe? no$,alm$ | no$,alm$,A$
:SLP2:TIMe no$,alm$,hour,min,sec,ms | alm$ = no$ = hour = 0～23(hour) min = 0～59(min) sec = 0～59(sec) ms = 0～999(millisec) | Sets the time of alarm change amount Queries
:SLP2:TIMe? no$,alm$ | no$,alm$,hour<NR1>,min<NR1>,sec<NR1>,ms<NR1>
:STIMe no$,alm$,hour,min,sec | no$ = alm$ = hour = 0 to 6(hour) min = 0 to 59(min) sec = 0 to 59(sec) | Sets time width of slope alarm Queries
:STIMe? no$,alm$ | no$,alm$,hour<NR1>,min<NR1>,sec<NR1>
:UPPEr no$,alm$,A | no$ = alm$ = A = upper limit level | Sets upper limit level of window-in/-out alarm Queries
:UPPEr? no$,alm$ | no$,alm$,A<NR3> (3 decimal places)
Pulse Channel Alarm (:ALARm:PULSe)
:KIND alm$,pls$,A$ | alm$ = pls$ = A$ = OFF, LEVEl, WINDow, SLOPe, SLOPE2 | Sets type of alarm Queries
:KIND? alm$,pls$ | alm$,pls$,A$
:LEVEl alm$,pls$,A | alm$ = pls$ = A = 0 to 1000000000(COUNT) 0 to 15000(r/s) 0 to 900000(r/min) | Sets the alarm level of the level alarm Queries
:LEVEl? pls$ | pls$,A<NR3> (9 decimal places)
:LOWEr alm$,pls$,A | alm$ = pls$ = A = 0 to 1000000000(COUNT) 0 to 15000(r/s) 0 to 900000(r/min) | Sets lower limit level of window-in/-out alarm Queries
:LOWEr? alm$,pls$ | alm$,pls$,A<NR3> (9 decimal places)
:SIDE alm$,pls$,A$ | alm$ = pls$ = A$ = IN, OUT | Sets the alarm side(window alarm) Queries
:SIDE? alm$,pls$ | alm$,pls$,A$
:SLOPe alm$,pls$,A$ | alm$ = pls$ = A$ = HIGH, LOW | Sets the alarm slope(level alarm) Queries
:SLOPe? alm$,pls$ | alm$,pls$,A$
:SLP2:TIMe alm$,pls$,hour,min,sec,ms | alm$ = pls$ = hour = 0～23(hour) min = 0～59(min) sec = 0～59(sec) ms = 0～999(millisec) | Sets the time of alarm change amount Queries
:SLP2:TIMe? alm$,pls$ | alm$,pls$,hour<NR1>,min<NR1>,sec<NR1>,ms<NR1>
:STIMe alm$,pls$,hour,min,sec | alm$ = pls$ = hour = 0 to 6(hour) min = 0 to 59(min) sec = 0 to 59(sec) | Sets time width of slope alarm Queries
:STIMe? alm$,pls$ | alm$,pls$,hour<NR1>,min<NR1>,sec<NR1>
:UPPEr alm,pls$,A | alm$ = pls$ = A = 0 to 1000000000(COUNT) 0 to 15000(r/s) 0 to 900000(r/min) | Sets upper limit level of window-in/-out alarm Queries
:UPPEr? alm$,pls$ | alm$,pls$,A<NR3> (9 decimal places)
Logic Channel Alarm (:ALARm:LOGic)
:ANDOR alm$,A$ | alm$ = A$ = OFF, OR, AND | Sets AND/OR for the logic alarm pattern Queries
:ANDOR? alm$ | alm$,A$
:PATTern alm$,"A$" | alm$ = A$ = xxxxxxxx alarm pattern(X, 0, 1) | Sets the pattern for a logic alarm
:PATTern? alm$ | alm$,"A$"