Scaling setting (SCALing)

Sets and queries the type of scaling.
Syntax | (Command) (Query) | :SCALing:KIND ch$,A$ :SCALing:KIND? ch$
(Response) | ch$,A$ ch$ = , A$ = RATIO, POINT, RATED, SENS
Details | Sets the type of scaling designated by ch$. Returns the current type of scaling designated by ch$ as a character string.
RATIO | Scale by specifying a conversion ratio
POINT | Scale by specifying two data points
RATED | Scale in terms of rated output
SENS | Scale by specifying a sensitivity
Example | :SCALing:KIND CH1_1,POINT :SCALing:KIND? CH1_1 (Response) :SCALING:KIND CH1_1,POINT (when headers are enabled)
Note | The setting method depends on the unit type.
Usage Conditions | -

Sets and queries the scaling offset.
Syntax | (Command) (Query) | :SCALing:OFFSet ch$,A :SCALing:OFFSet? ch$
(Response) | ch$,A<NR3> (4 decimal places) ch$ = , A = -9.9999E+09 to 9.9999E+09
Details | Sets the scaling offset for the channel designated by ch$. Returns the current scaling offset for the channel designated by ch$ as an NR3 numerical value.
Example | :SCALing:OFFSet CH1_1,0 :SCALing:OFFSet? CH1_1 (Response) :SCALING:OFFSET CH1_1,+0.0000E+00 (when headers are enabled)
Note | The possible values for A are the same as for the main unit. This setting may change the following settings Scaling SCALE UP and LOW Thresholds for Numerical Calculation
Usage Conditions | -

Sets and queries scaling rated capacity.
Syntax | (Command) (Query) | :SCALing:RTDCapa ch$,A :SCALing:RTDCapa? ch$
(Response) | ch$,A<NR3> (4 decimal places) ch$ = A = +1.0000E-09 to +9.9999E+09
Details | Sets the scaling rated capacity for the channel designated by ch$. Returns the current scaling rated capacity for the channel designated by ch$ as an NR3 numerical value.
Example | :SCALing:RTDCapa CH1_1,2 :SCALing:RTDCapa? CH1_1 (Response) :SCALING:RTDCAPA CH1_1,+2.0000E+00 (when headers are enabled)
Note | The configurable range of scaling rated capacity may vary depending on the setting of the scaling rated output. This setting may change the following settings Scaling SCALE UP and LOW Scaling sense value Scaling conversion value
Usage Conditions | Strain unit (U8554, LR8534)

Sets and queries scaling rated output.
Syntax | (Command) (Query) | :SCALing:RTDOut ch$,A :SCALing:RTDOut? ch$
(Response) | ch$,A<NR3> (4 decimal places) ch$ = A = +1.0000E-09 to +9.9999E+09
Details | Sets the scaling rated output for the channel designated by ch$. Returns the current scaling rated output for the channel designated by ch$ as an NR3 numerical value.
Example | :SCALing:RTDOut CH1_1,1 :SCALing:RTDOut? CH1_1 (Response) :SCALING:RTDOUT CH1_1,+1.0000E+00 (when headers are enabled)
Note | The configurable range of scaling rated output may vary depending on the setting of the scaling rated capacity. This setting may change the following settings Scaling SCALE UP and LOW Scaling sense value Scaling conversion value
Usage Conditions | Strain unit (U8554, LR8534)

Sets and queries the scaling SCALE UP and LOW.
Syntax | (Command) (Query) | :SCALing:SCUPLOw ch$,A,B :SCALing:SCUPLOw? ch$
(Response) | ch$,A<NR3>,B<NR3> (4 decimal places) ch$ = , A, B = -9.9999E+29 to +9.9999E+29
Details | Sets the scaling SC UP and SC LOW values for the channel designated by ch$. Returns the current scaling SC UP and SC LOW values for the channel designated by ch$ as an NR3 numerical value.
Example | :SCALing:SCUPLOw CH1_1,0.5,-0.5 :SCALing:SCUPLOw? CH1_1 (Response) :SCALING:SCUPLOW CH1_1,+5.0000E-01,-5.0000E-01 (when headers are enabled)
Note | Same value in A and B can not be set. This setting may change the following settings Scaling offset Scaling rated capacity Scaling rated output Scaling sense value Scaling conversion value
Usage Conditions | -

Sets and queries the scaling sense value.
Syntax | (Command) (Query) | :SCALing:SENSE ch$,A :SCALing:SENSE? ch$
(Response) | ch$,A<NR3> (4 decimal places) ch$ = , A = -1.0000E+09 to +1.0000E+09
Details | Sets the scaling sense value for the channel designated by ch$. Returns the current scaling sense value setting for the channel designated by ch$ as an NR3 numerical value.
Example | :SCALing:SENSE CH1_1,1 :SCALing:SENSE? CH1_1 (Response) :SCALING:SENSE CH1_1,+1.0000E+00 (when headers are enabled)
Note | The possible values for A are the same as for the main unit. This setting may change the following settings Scaling rated capacity Scaling rated output Scaling SCALE UP and LOW Scaling conversion value
Usage Conditions | -

Sets and queries the scaling kind.
Syntax | (Command) (Query) | :SCALing:SET ch$,A$ :SCALing:SET? ch$
(Response) | ch$,A$ ch$ = , A$ = OFF, ENG, SCI
Details | Sets the scaling kind designated by ch$. Returns the current scaling kind designated by ch$ as a character string.
OFF | Scaling is disabled
ENG | Decimal: Scaling is enabled and values are displayed using engineering notation
SCI | Exponential: Scaling is enabled and values are displayed using scientific notation
Example | :SCALing:SET CH1_1,ENG :SCALing:SET? CH1_1 (Response) :SCALING:SET CH1_1,ENG (when headers are enabled)
Note | -
Usage Conditions | -

Sets and queries the scaling unit.
Syntax | (Command) (Query) | :SCALing:UNIT ch$,"A$" :SCALing:UNIT? ch$
(Response) | ch$,"A$" ch$ = , A$ = scaling unit (up to 7 characters)
Details | Sets the scaling unit for the channel designated by ch$. Returns the current scaling unit for the channel designated by ch$ as character data. Single quotation marks (') can be used instead of double quotation marks("). Entry of the special characters is as follows.
PC | ^2 | ^3 | ~u | ~o | ~e | ~c | ~+ | ~, | ~; | ^^ | ~~
LR8450 LR8450-01 | 2 | 3 | μ | Ω | ε | ° | ± | ' | " | ˆ | ˜
Example | :SCALing:UNIT CH1_1,"mA" :SCALing:UNIT? CH1_1 (Response) :SCALING:UNIT CH1_1,"mA" (when headers are enabled)
Note | Characters exceeding the maximum number of characters are not set.
Usage Conditions | -

Sets and queries the scaling conversion value.(RATIO)
Syntax | (Command) (Query) | :SCALing:VOLT ch$,A :SCALing:VOLT? ch$
(Response) | ch$,A<NR3> (4 decimal places) ch$ = , A = -9.9999E+09 to +9.9999E+09 (pulse channel mode = COUNT:+1.0000E-09 to +9.9999E+09)
Details | Sets the scaling conversion value for the channel designated by ch$. Returns the current scaling conversion value setting for the channel designated by ch$ as an NR3 numerical value.
Example | :SCALing:VOLT CH1_1,1 :SCALing:VOLT? CH1_1 (Response) :SCALING:VOLT CH1_1,+1.0000E+00 (when headers are enabled)
Note | The possible values for A are the same as for the main unit. This setting may change the following settings Scaling rated capacity Scaling rated output Scaling SCALE UP and LOW Scaling sense value
Usage Conditions | -

Sets and queries the scaling VOLT UP and LOW.
Syntax | (Command) (Query) | :SCALing:VOUPLOw ch$,A,B :SCALing:VOUPLOw? A$
(Response) | ch$,A<NR3>,B<NR3> (4 decimal places) ch$ = , A, B = -9.9999E+29 to +9.9999E+29
Details | Sets the scaling VOLT UP and VOLT LOW values for the channel designated by ch$. Returns the current scaling VOLT UP and VOLT LOW values for the channel designated by ch$ as an NR3 numerical value.
Example | :SCALing:VOUPLOw CH1_1,0.05,-0.05 :SCALing:VOUPLOw? CH1_1 (Response) :SCALING:VOUPLOW CH1_1,+5.0000E-02,-5.0000E-02 (when headers are enabled)
Note | Same value in A and B can not be set. This setting may change the following settings Scaling offset Scaling rated capacity Scaling rated output Scaling sense value Scaling conversion value
Usage Conditions | -